Data/hora: 01/06/2024 14:00:12

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 05/04/2005
Data da última atualização: | 05/04/2005
Autoria: | MEDEIROS, E. S.; AGNELLI, J. A. M.; JOSEPH, K.; CARVALHO, L. H.; MATTOSO, L. H. C.
Título: | Curing behavior of a Novolac-type phenolic resin analyzed by differential scanning calorimetry.
Ano de publicação: | 2003
Fonte/Imprenta: | Journal of applied polymer science, v. 90, p.g 1678-1682, 2003.
Idioma: | Inglês

Conteúdo:

Phenolic resins are widely used condensation poly- mers because of their high chemical resistance, electri- cal insulation, and dimensional stability. Their roain applications include molding materiaIs, laminates, and adhesives in the manufacture of plywood.1 
There are two major categories of phenolic resins that are classified by their structures and curing prop- erties as resole or novolac. The essential characteristics of both cured resole and novolac-type phenolic resins are almost identical (e.g., mechanical properties, chemical resistance, etc.).

Palavras-Chave: | DSC; Método Ozawa; Microgel; Resinas fenólicas.
Thesaurus Nal: | differential scanning calorimetry.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (8786-1) - UPC - SP - -- - PROCI-03.00131 -  - 2003.00131 - DIS