Data/hora: 14/06/2024 16:23:37

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	06/01/2014	
Data da última atualização: 	12/12/2016	
Autoria: 	SAMUEL-ROSA, A.; ANJOS, L. H. C. dos; VASQUES, G. de M.; ANTUNES, M. A. H.; DALMOLIN, R. S. D.	
Afiliação: 	Alessandro Samuel-Rosa, UFRRJ; Lúcia H. C. dos Anjos, UFRRJ; GUSTAVO DE MATTOS VASQUES, CNPS; Mauro A. H. Antunes, UFRRJ; Ricardo S. D. Dalmolin, UNIVERSIDADE FEDERAL DE SANTA MARIA.	
Título: 	Identifying and correcting oblique striping in the topodata digital elevation model.	
Ano de publicação: 	2013	
Fonte/Imprenta: 	In: CONGRESSO BRASILEIRO DE CIÊNCIA DO SOLO, 34., 2013, Florianópolis. Anais... Florianópolis: Sociedade Brasileira de Ciência do Solo, 2013.	
Idioma: 	Inglês	
Conteúdo: 	The Topodata digital elevation model (DEM) is the best DEM available for digital soil mapping (DSM) in Brazil. However, it is not ready to use. We show that the kriging interpolator used to downscale the SRTM DEM from 3 arc-seconds to 1 arc-second spatial resolution increased the double oblique striping (15º and 60º) so common to SRTM DEMs. This is because kriging is quite sensitive to outliers. Besides, the Gaussian model of spatial covariance used in the downscaling enhanced the sensitivity of kriging to outliers, thus enhancing the striping. 2D Fast Fourier Transform can be used to identify whether a destriping procedure need to be employed. The bilinear or cubic resampling methods should be used to warp Topodata DEMs because they are insensitive to the double oblique striping.	
Palavras-Chave: 	2D Fast Fourier Transform; DEM warping; SRTM downscaling.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/94694/1/identifying.pdf	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (17880-1) - UPC - AA - DD - 14.00008 -  - 14.00008 - DIS