Data/hora: 05/06/2024 01:44:15

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 03/02/2006
Data da última atualização: | 03/02/2006
Autoria: | VENANCIO, E. C.; PATERNO, L. G.; CONSOLIN FILHO, N.; BORATO, C. E.; FIRMINO, A.; MATTOSO, L. H.
Título: | Influence of the pH and substrate immersion time on the adsorption of Poly(o-ethoxyaniline) in self-assembled films.
Ano de publicação: | 2005
Fonte/Imprenta: | Journal of the Brazilian Chemical Society, São Paulo, v. 16, n. 3B, p. 558-564, 2005.
Idioma: | Inglês
Conteúdo: | Ultra-thin films of poly(o-ethoxyaniline)- POEA were deposited onto quartz slides by the self-assembly technique from aqueous solutions of this polymer in pH 3 and 5. The influence of the experimental conditions on the amount of POEA adsorbed was evaluated bu UV-Vis spectroscopy, atomic force microscopy and cyclic voltammetry.
Palavras-Chave: | Conducting polymers; Poly(o-ethoxyaniline); Self-assembled films; Thin films.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9383-1) - UPC - SP - -- - PROCI-05.00122 -  - 2005.00122 - DIS