Data/hora: 08/06/2024 20:58:40

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	29/09/2014	
Data da última atualização: 	08/11/2021	
Autoria: 	SANTOS, V. B. dos; FAVA, E. L.; PESSOA-NETO, O. D.; BIANCHI, S. R.; FARIA, R. C.; FATIBELLO-FILHO, O.	
Afiliação: 	Vagner Bezerra dos Santos, Universidade Federal de São Carlos; Elson Luiz Fava, Universidade Federal de São Carlos; Osmundo Dantas Pessoa-Neto, Universidade Federal de São Carlos; SILMARA ROSSANA BIANCHI, CNPS; Ronaldo Censi Faria, Universidade Federal de São Carlos; Orlando Fatibello-Filho, Universidade Federal de São Carlos.	
Título: 	A versatile and robust electrochemical flow cell with a boron-doped diamond electrode for simultaneous determination of Zn2+ and Pb2+ ions in water samples.	
Ano de publicação: 	2014	
Fonte/Imprenta: 	Analytical Methods, v. 6, p. 8526-8534, 2014.	
DOI: 	https://doi.org/10.1039/C4AY01811G	
Idioma: 	Inglês	
Conteúdo: 	A versatile and robust thermostatted electrochemical flow cell (EFC) with a boron-doped diamond electrode (BDD) detector was employed to perform two distinct flow-injection electrochemical approaches. In the first approach, differential pulse anodic stripping voltammetry (DPASV) using a flowbatch analysis (FBA) is proposed. In the second approach, multiple pulse amperometry (MPA) employing multicommutation flow analysis (MCFA) is also presented. Both approaches were employed to simultaneously determine Zn2+ and Pb2+ in water samples. For this, a screen-printed electrode (SPE) was developed, and a BDD electrode was coupled to it and was inserted into the EFC. By employing the FBA with the DPASV technique, two analytical curves in concentration ranges from 11.5 to 80.6 mg L1 and 0.64 to 10.9 mg L1 for simultaneous determination of Zn2+ and Pb2+, respectively, were obtained. Moreover, limits of detection (LDs) of 0.62 mg L1 and 0.19 mg L1 were estimated respectively and a sampling frequency of 12 h1 was obtained. For MCFA with MPA, analytical curves from 830 to 4980 mg L1 and 140 to 820 mg L1 for simultaneous determination of Zn2+ and Pb2+ with LDs of 220.0 mg L1 and 41.0 mg L1 and a sampling frequency of 67 h1 were obtained. The developed EFC allowed a full on-line automation of the methods, covering the pretreatment of BDD, addition of standard solutions, dilutions, thermostatted control, and detection with and without electrochemical preconcentration. In addition, the low waste generation of only 700 mL may be useful for green chemistry purposes and sustainable research.	
Palavras-Chave: 	Diamond eletrode; Eletrodo de diamante; Pb2+; Zn2+.	
Thesagro: 	Boro.	
Thesaurus Nal: 	boron.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (18491-1) - UPC - AP - DD -  -  - 2014.00685 - DIS