Data/hora: 03/06/2024 03:44:17

Biblioteca(s): 	Embrapa Mandioca e Fruticultura.	
Data corrente: 	06/07/1995	
Data da última atualização: 	06/07/1995	
Autoria: 	COHEN, Y.; MORESHET, S.; FUCHS, M.	
Afiliação: 	Departament of Agricultural Meteorology, Institute of Soils and Water,Bet Dagan, Israel.	
Título: 	changes in hydraulic conductance of citrus trees following a reduction in wetted soil volume.	
Ano de publicação: 	1987	
Fonte/Imprenta: 	Plant, Cell and Environment, v.10, p.53-57, 1987.	
Idioma: 	Inglês	
Conteúdo: 	The effect of the transition from fully to partially wetted soil volume on transpiration rate and hydraulic conductance of mature citrus trees was examined in a 23-year-old, commercial, sprinkler-irrigated, Shamouti orange orchard. Irrigation frequency was determined by the rate of water loss from the soil, as measured by neutron probes. The hydraulic conductance of the tree was computed from the relationship betweensap flow in the trunk and leaf potential. The diurnal values of leaf water potential and sap flow shifted towards lower levels as the water stored in the root zone was depleted.	
Palavras-Chave: 	Citrus sinesis L; Osbeck; Transpirtation.	
Thesaurus Nal: 	water potential.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Mandioca e Fruticultura (CNPMF)	
Exemplares: 	CNPMF - (16076-1) - ADC - SP - -- -  -  - S9835 - DIS