Data/hora: 14/06/2024 00:33:21

Biblioteca(s): 	Embrapa Pantanal.	
Data corrente: 	18/10/1995	
Data da última atualização: 	07/04/2017	
Autoria: 	SIPPEL, S. J.; HAMILTON, S. K.; MELACK, J. M.; CHOUDHURY, B. J.	
Título: 	Determination of inundation area in the Amazon River floodplain using the SMMR 37 GHz polarization difference.	
Ano de publicação: 	1994	
Fonte/Imprenta: 	Remote Sensing Environment, v.48, p.70-76, 1994.	
Idioma: 	Inglês	
Conteúdo: 	The 37 GHz polarization difference observed by the Scanning Multichannel Microwage Radiometer (SMMR), which was operated on board the Nimbus-7 satellite, provides a sensitive indicator of surface water. These data can provide information on seasonal inundation patterns in large tropical wetlands such as the Amazon River flodplain. Although the SMMR data are of low resolution, we were able to estimate the area inundated within a group of pixels by using linear mixing models which incorporate the major end-members of the observed microwage signatures. The models were then used to estimate seasonal changes in inundation area over a 7-year period for a 34,550 km2 area along the Amazon River near Manaus. The seasonal changes in inundation area determined using mixing models correlate well with changes in river stage.	
Palavras-Chave: 	Floresta Amazonica; Inundation; Rio Amazonas.	
Thesagro: 	Inundação; Limnologia; Sensoriamento Remoto.	
Thesaurus Nal: 	Amazon River; limnology; remote sensing.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Pantanal (CPAP)	
Exemplares: 	CPAP - (30097-1) - ADD - SP - PP - SP14665 -  - 14665 - DIS