Data/hora: 05/06/2024 00:36:05

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 28/03/2006
Data da última atualização: | 28/03/2006
Autoria: | VASQUES, R. A.; INNOCENTINI, M. D. M.; ASSIS, O. B. G.
Título: | A simple apparatus for determining the permeability of thin-thickness porous materials by pressure-decay technique.
Ano de publicação: | 1999
Fonte/Imprenta: | Revista de Física Aplicada e Instrumentação, Rio de Janeiro, v.14, n.4, p.120-123, dez. 1999.
Idioma: | Inglês
Conteúdo: | A simple experimental set up, for the evaluation of the permeability of thin-thickness porous material, is presented. The proposed system makes use of a perpendicular fluid flux that at controlled pressure can permeate the medium.The permeability variables are estimated by measuring the relative pressure before and after the fluid permeates the sample.
Palavras-Chave: | Materiais porosos; Membranas vítreas.
Thesagro: | Permeabilidade.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9679-1) - UPC - SP - -- - PROCI-99.00155 -  - 1999.00155 - DIS