Data/hora: 09/06/2024 23:25:19

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 26/08/2020
Data da última atualização: | 16/08/2022
Autoria: | FARIA, D. L.; MESQUITA JUNIOR, L.; RESENDE, A. A.; LOPES, D. E.; MENDES, L. M.; MARTINS, M. A.; MARCONCINI, J. M.; GUIMARÃES JUNIOR, J. B.
Afiliação: | MARIA ALICE MARTINS, CNPDIA; JOSE MANOEL MARCONCINI, CNPDIA.
Título: | Physical and mechanical properties of polyurethane thermoset matrices reinforced with green coconut fibres.
Ano de publicação: | 2020
Fonte/Imprenta: | Journal of Composite Materials, v. 54, n. 30, 2020.
Páginas: | 4841-4852
DOI: | 10.1177/0021998320940023
Idioma: | Inglês
Conteúdo: | Currently, the use of composites to replace parts made only with plastics has been gradually employed. The advantages of these composites are low cost, high availability of raw materials and good physical and mechanical properties. Thus, this work aimed at producing and characterizing composites produced with coconut fibre reinforced polyurethane matrices. The coconut fibres were studied as to their chemical constituents, aspect ratio, bulk density, pH, tensile properties, and surface SEM images. The composites were prepared using the hand lay-up process and four different concentrations of coconut fibre were evaluated: 30, 40, 50, and 60%. The composites were assessed as for water absorption after 20 days of immersion, bulk density, impact IZOD, tensile tests, and visualize the matrix-reinforcement interface using SEM. The electron micrographs showed a great deal of impurities on the surface of coconut fibres, such as greases, waxes, and gums, due to the high amount of extraction material (19.78%), which damages the adherence of the polymer onto the coconut fibre and, as observed, cause detachment between the reinforcement and the matrix. The tensile strength of the composites tended to increase as greater amounts of coconut fibres were added to the matrix. The averages were around 6.51 to 6.72 MPa for composites with 30 and 60% fibres, respectively. Therefore, coconut fibres can be considered as an alternative to synthetic fibres commonly used in composites, and they can be used at a ratio of 60% without prejudicing the properties of the composites, making them lighter and cheaper.
Palavras-Chave: | Thermoset matrices.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (17568-1) - UPC - AP - DD - PROCI.20/052 -  - 2020/0058 - DIS