Data/hora: 01/06/2024 18:09:56

Biblioteca(s): 	Embrapa Gado de Leite.	
Data corrente: 	22/12/2017	
Data da última atualização: 	27/01/2023	
Autoria: 	MENDONÇA, H. V. de; OMETTO, J. P. H. B.; OTENIO, M. H.; REIS, A. J. D. dos; MARQUES, I. P. R.	
Afiliação: 	UFJF; UFJF; MARCELO HENRIQUE OTENIO, CNPGL; Campus Lumiar - Lisboa; Campus Lumiar - Lisboa.	
Título: 	Bioenergy recovery from cattle wastewater in an UASB-AF hybrid reactor.	
Ano de publicação: 	2017	
Fonte/Imprenta: 	Water Science & Technology, v. 76, n. 9, p. 2268-2279, 2017.	
Idioma: 	Inglês	
Conteúdo: 	ABSTRACT New data on biogas production and treatment of cattle wastewater were registered using an upflow anaerobic sludge blanket-anaerobic filter (UASB-AF) hybrid reactor under mesophilic temperature conditions (37 WC). The reactor was operated in semi-continuous mode with hydraulic retention times of 6, 5, 3 and 2 days and organic loading rates of 3.8, 4.6, 7.0 and 10.8 kg CODt m3 d1. Biogas volumes of 0.6?0.8 m3 m3 d1 (3.8?4.6 kg CODt m3 d1) and 1.2?1.4 m3 m3 d1 (7.0?10.8 kg CODt m3 d1), with methane concentrations between 69 and 75%, were attained. The removal of organic matter with values of 60?81% (CODt) and 51?75% (CODs) allowed methane yields of 0.155?0.183 m3 CH4 kg1 CODt and 0.401?0.513 m3 CH4 kg1 CODs to be obtained. Volatile solids were removed in 34 to 69%, with corresponding methane yields of 0.27 to 0.42 m3 CH4 kg1 VSremoved. The good performance of the novel hybrid reactor was demonstrated by biogas outputs higher than reported previously in the literature, along with the quality of the gas obtained in the various experimental phases. The hybrid reactor investigated in this study presents comparative advantages, particularly in relation to conventional complete mixture units, considering economic factors such as energy consumption, reactor volume and installation area.	
Palavras-Chave: 	Cattle wastewater; UASB-AF hybrid reactor.	
Thesagro: 	Biogás.	
Thesaurus Nal: 	anaerobic digestion; bioenergy.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (23790-1) - UPC - AP - DD -  -  -  - DIS