Data/hora: 08/06/2024 12:28:50

Biblioteca(s): | Embrapa Gado de Leite.
Data corrente: | 16/08/2021
Data da última atualização: | 16/08/2021
Autoria: | SOUZA, D. S. de; MACIEL, A. M.; OTENIO, M. H.; MENDONCA, H. V. de.
Afiliação: | DENISE SALVADOR DE SOUZA, Universidade Federal Rural do Rio de Janeiro; ALYNE MARTINS MACIEL, Pós graduanda, Universidade Federal de Juiz de Fora; MARCELO HENRIQUE OTENIO, CNPGL; HENRIQUE VIEIRA DE MENDONÇA, Universidade Federal Rural do Rio de Janeiro.
Título: | Optimization of ozone application in post-treatment of cattle wastewater from organic farms.
Ano de publicação: | 2020
Fonte/Imprenta: | Water, Air and Soil Pollution, v. 231, 362, 2020.
DOI: | https://doi.org/10.1007/s11270-020-04736-2
Idioma: | Inglês
Conteúdo: | In this study, an advanced oxidation process using ozone application in a fixed-bed reactor filled with bio-rings was used for purification and disinfection of cattle wastewater (CWW) previously treated in a UASB reactor. The O3 concentration applied to the reactor was 7.8 mg L&#8722;1 (±1). Four ozonation times were tested in a batch process: T1 = 0.5 h, T2 = 1 h, T3 = 1.5 h and T4 = 2 h. The pH values tended to increase with the time of contact between liquid and gas. COD and BOD5 removal of 55 and 64% was recorded in T4. Color and turbidity were reduced by 88.5 and 93.4%, while total solids and total suspended solids were reduced by 65.7 and 93.5%, respectively. Oils and greases were completely removed from the wastewater. Electrical conductivity did not vary significantly between treatments, and its association with the presence of cations, such as Na+,Ca2+ and Mg2+, suggests good quality of the water ozonated in T4 for application in the soil, with no risk of salinization. High concentrations of nitrogen compounds were removed, but the efficiency in removing phosphate compounds was low. Coliform removal of above 99% was achieved with T3. Only the CWW ozonated in T4 is recommended for irrigation of rawconsumed crops. Based on most parameters analyzed, the CWW treated in T4 would also be suitable for discharge into water bodies according to Brazilian legislation, suggesting that this technology could be applied in the near future.
Palavras-Chave: | Coliformremoval; Esgoto bovino; Oxidação avançada; Reuse; Rural sanitation.
Thesagro: | Bovino; Coliforme; Gado; Oxidação; Ozônio; Saneamento Rural.
Thesaurus Nal: | Advanced oxidation protein products.
Categoria do assunto: | L Ciência Animal e Produtos de Origem Animal
Registro original: | Embrapa Gado de Leite (CNPGL)
Exemplares: | CNPGL - (25219-1) - UPC - AP - DD -  -  -  - DIS