Data/hora: 31/05/2024 18:24:09

Biblioteca(s): 	Embrapa Pesca e Aquicultura.	
Data corrente: 	06/12/2017	
Data da última atualização: 	06/12/2017	
Autoria: 	MOREIRA, R. F. P. M.; VANDRESEN, S.; LUIZ, D. B.; JOSÉ, H. J.; LI PUMA, G.	
Afiliação: 	REGINA F. P. M. MOREIRA, UNIVERSIDADE FEDERAL DE SANTA CATARINA; SOLANGE VANDRESEN, UNIVERSIDADE FEDERAL DE SANTA CATARINA; DANIELLE DE BEM LUIZ, CNPASA; HUMBERTO J. JOSE, UNIVERSIDADE FEDERAL DE SANTA CATARINA; GIANLUCA LI PUMA, LOUGHBOROUGH UNIVERSITY, United Kingdom.	
Título: 	Adsorption of arsenate, phosphate and humic acids onto acicular goethite nanoparticles recovered from acid mine drainage.	
Ano de publicação: 	2017	
Fonte/Imprenta: 	Journal of Environmental Chemical Engineering, v. 5, p. 652-659, 2017.	
ISSN: 	2213-3437	
DOI: 	10.1016/j.jece.2016.12.018	
Idioma: 	Inglês	
Conteúdo: 	Acicular goethite nanoparticles (AGNs), obtained from the active treatment of acid mine drainage (AMD) on an industrial scale, were evaluated with respect to their capacity to adsorb the contaminants arsenate, phosphate and humic acids (HAs) in aqueous solution. Kinetics and equilibrium constants that describe the adsorption process were investigated. The adsorption capacity decreased in the order: HAs (37 mgC g!1) > As(V) (20 mg As(V) g!1) > phosphate ions (13 mgPO4 3! g!1). The adsorption capacity of the AGNs produced from acid mine drainage to remove arsenate, phosphate or humic acids are similar to those found for other synthetic iron oxides produced under controlled conditions at the laboratory scale. This study demonstrates the valorization of the AGNs product derived from acid mine drainage slurry waste arising from the mining of coal as an effective adsorbent materials for water treatment.	
Palavras-Chave: 	Iron ioxides.	
Thesaurus Nal: 	Adsorption; Water treatment.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Pesca e Aquicultura (CNPASA)	
Exemplares: 	CNPASA - (595-1) - UPC - AP - DD - CNPASA_AP66 -  - 2017.066 - DIS