Data/hora: 01/06/2024 14:20:26

Biblioteca(s): | Embrapa Solos.
Data corrente: | 04/01/2010
Data da última atualização: | 16/09/2021
Autoria: | RAMOS, P. F. de O.; TOLEDO, I. B. de; NOGUEIRA, C. M.; NOVOTNY, E. H.; VIEIRA, A. J. M.; AZEREDO, R. B. de V.
Afiliação: | PAULO FREDERICO DE OLIVEIRA RAMOS, PETROBRAS; INGRID BERTONI DE TOLEDO, UFF; CHRISTIANE MAPHEU NOGUEIRA, UFF; ETELVINO HENRIQUE NOVOTNY, CNPS; ALEXANDRE JAIME MELLO VIEIRA, PETROBRAS; RODRIGO BAGUEIRA DE VASCONCELLOS AZEREDO, UFF.
Título: | Low field 1H NMR relaxometry and multivariate data analysis in crude oil viscosity prediction.
Ano de publicação: | 2009
Fonte/Imprenta: | Chemometrics and Intelligent Laboratory Systems, v. 99, n. 2, p. 121-126, Dec. 2009.
DOI: | https://doi.org/10.1016/j.chemolab.2009.08.001
Idioma: | Inglês
Conteúdo: | This study explores the application of multivariate data analysis in the viscosity prediction of crude oils using NMR relaxation data. The 1H transverse relaxation times (T2) of 68 Brazilian crude oil samples, ranging from light to extra-heavy (2 to 30,000 cP), were measured at 2 MHz. Partial least squares regression (PLSR) models were developed to predict the oil viscosity in log viscosity units from the T2 relaxation spectra and directly from the raw relaxation curves. In both cases, the PLSR with only three latent variables produced good calibration models, with a standard error of prediction of 0.161 and 0.135 log cP for the T2 relaxation spectra and raw relaxation curves, respectively. The PLSR models were validated by full cross and external set schemes revealing quite equivalent performances.
Palavras-Chave: | Óleo cru; PLSR.
Thesagro: | Viscosidade.
Categoria do assunto: | P Recursos Naturais, Ciências Ambientais e da Terra
Registro original: | Embrapa Solos (CNPS)
Exemplares: | CNPS - (14411-1) - UPC - AP - DD -  -  - 2009.00176 - DIS