Data/hora: 05/06/2024 01:06:12

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 05/06/2020
Data da última atualização: | 16/08/2022
Autoria: | SOARES, A. C.; SOARES, J. C.; PASCHOALIN, R. T.; RODRIGUES, V. C.; MELENDEZ, M. E.; REIS, R. M.; CARVALHO, A. L.; MATTOSO, L. H. C.; OLIVEIRA, O. N.
Afiliação: | LUIZ HENRIQUE CAPPARELLI MATTOSO, CNPDIA.
Título: | Immunosensors containing solution blow spun fibers of poly(lactic acid) to detect p53 biomarker.
Ano de publicação: | 2020
Fonte/Imprenta: | Materials Science & Engineering C, v. 115, 2020.
Páginas: | 1-10
ISSN: | 0928-4931
DOI: | https://doi.org/10.1016/j.msec.2020.111120
Idioma: | Inglês
Conteúdo: | This paper reports on biosensors made with a matrix of polylactic acid (PLA) fibers, which are suitable for immobilization of the anti-p53 active layer for detection of p53 biomarker. The PLA fibers were produced with solution blow spinning, a method that is advantageous for its simplicity and possibility to tune the fiber properties. For the biosensors, the optimized time to deposit the fibers was 60 s, with which detection of p53 could be achieved with the limit of detection of 11 pg/mL using electrical impedance spectroscopy. This sensitivity is also sufficient to detect the p53 biomarker in patient samples, which was confirmed by distinguishing samples from cell lines with distinct p53 concentrations in a plot where the impedance spectra were visualized with the interactive document mapping (IDMAP) technique. The high sensitivity and selectivity of the biosensors may be attributed to the specific interaction between the active layer and p53 modeled with a Langmuir-Freundlich and Freundlich isotherms and inferred from the analysis of the vibrational bands at 1550, 1650 and 1757 cm&#8722;1 using polarization-modulated infrared reflection absorption spectroscopy (PM-IRRAS). The successful immobilization of the active layer is evidence that the approach based on solution blown spun fibers may be replicated to other types of biosensors.
Palavras-Chave: | Immunosensor; PLA fibers; Solution blow spinning.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (17550-1) - UPC - AP - DD - PROCI.20/039 -  - 2020/044 - DIS