Data/hora: 03/06/2024 03:47:29

Biblioteca(s): 	Embrapa Suínos e Aves.	
Data corrente: 	23/05/2016	
Data da última atualização: 	22/02/2017	
Autoria: 	PIROLLI, M.; SILVA, M. L. B. da; MEZZARI, M. P.; MICHELON, W.; PRANDINI, J. M.; SOARES, H. M.	
Afiliação: 	MATEUS PIROLLI, UFSC; MARCIO LUIS BUSI DA SILVA, CNPSA; MELISSA PAOLA MEZZARI, UNOESC; WILLIAN MICHELON, UFSC; JEAN MICHEL PRANDINI, UFSC; HUGO MOREIRA SOARES, UFSC.	
Título: 	Assessment of hydrogen sulfide removal from biogas using a field scale anoxic biotrickling filter.	
Ano de publicação: 	2015	
Fonte/Imprenta: 	In: LATIN AMERICAN CONGRESS, 4., 2015, Florianópolis. Anais... Florianópolis: UFSC, 2015. Disponível on line. SOLABIAA.	
Idioma: 	Inglês	
Conteúdo: 	Hydrogen sulphide is one of the most toxic and corrosive compound present in swine-derived biogas streams.In this study, afield scale biotrickling filter for the removal of hydrogen sulfide was investigated.A Biofilter packed with supporting biofilm materials was fed continuously with a proprietary nutrient solution and operatedfor over 73days. The system has been operating with a H2S inlet concentrations ranging from 1,000to 3,000 ppm.Significant removal efficiencies >95% was demonstrated. pH of the stock feeding solution decreased from 6.2 to as low as 3.5within couple days.The resulting drop in pH provided circumstantial evidence to support biological H2 Soxidation to sulphuric acid by sulfide-oxidizers. Sulfur precipitation was also observed to occur. The results suggested that H2S removal from biogas stream can be efficiently achieved using portable, low cost and maintenance free biotrickling filters.	
Palavras-Chave: 	Biotrickling filter.	
Thesagro: 	Biogás.	
Thesaurus Nal: 	desulfurization; hydrogen sulfide.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/143245/1/final7859.pdf	
Registro original: 	Embrapa Suínos e Aves (CNPSA)	
Exemplares: 	CNPSA - (20623-1) - UPC - AA - DD -  -  -  - DIS