Data/hora: 17/05/2024 01:32:48

Biblioteca(s): 	Embrapa Agroenergia.	
Data corrente: 	16/11/2023	
Data da última atualização: 	16/11/2023	
Autoria: 	CARVALHO, L.; CORREA, I.; ALMEIDA, E. S.; SILVA, A. M. A.; VALADARES, L. F.; LUNA, F. M. T.; SILVA JUNIOR, I. J.; MONTEIRO, S.	
Afiliação: 	LAIANE CARVALHO, UNIVERSIDADE FEDERAL DE GOIAS; ISABELLA CORREA, UNIVERSIDADE DE BRASILIA; ERISLENE S. ALMEIDA, CNPAE; ALYSSON M. A. SILVA, UNIVERSIDADE DE BRASILIA; LEONARDO FONSECA VALADARES, CNPAE; F. MURILO T. LUNA, UNIVERSIDADE FEDERAL DO CEARÁ; IVANILDO J. SILVA JUNIOR, UNIVERSIDADE FEDERAL DO CEARÁ; SIMONE MONTEIRO, UNIVERSIDADE DE BRASILIA.	
Título: 	Recovering carotenes from crude palm oil onto macroporous polymeric resin: dynamic adsorption experiments and mechanistic insights.	
Ano de publicação: 	2023	
Fonte/Imprenta: 	Adsorption, October 2023.	
DOI: 	https://doi.org/10.1007/s10450-023-00419-6	
Idioma: 	Inglês	
Notas: 	Special Issue: EBA14 - 14th Brazilian Meeting on Adsorption. On-line first.	
Conteúdo: 	Abstract: This study aims to recover carotenes from crude palm oil, which are typically destroyed during refning, despite their high nutritional value and vitamin activity. The proposed approach involves the continuous adsorption of carotenes from crude palm oil onto polymeric resins, specifcally Diaion HP-20. To evaluate the adsorption process, breakthrough experiments were conducted using solutions consisting of 10% oil and 90% isopropanol (w/w) at a temperature of 313 K. The experimental data obtained from the breakthrough experiments were successfully predicted by a Linear Driving Force (LDF) model, indicating its adequacy in describing the adsorption process. The shape of the breakthrough curve was found to be signifcantly infuenced by the variation in axial dispersion (Dax). The estimated mass transfer coefcient (KL) varied from 2.25 for the fresh resin to 1.31 min&#8722;1 for the two-times regenerated, and the difusion in the adsorbate (DH) was 0.0202 mm2 /min; the average capacity of the solid phase was 0.78, 0.76 and 0.72 mg/g for fresh, one-time and two-time regenerated resins, respectively. FTIR analysis provided evidence of the formation of ester bonds between the polymeric resin and the oil, confrming the occurrence of chemical interactions during the adsorption process. MicroCT analysis indicates the presence of intraparticle difusion phenomena within the resin. A notable outcome of this study was the potential for reusing the polymeric resin for multiple cycles without a signifcant loss in its adsorptive capacity. This suggests the feasibility and promising nature of removing carotenes from crude palm oil through the proposed approach.	
Palavras-Chave: 	Força motriz linear; Microtomografia; Oleo comestível; Transferência de massa.	
Thesagro: 	Regeneração; Vitamina.	
Categoria do assunto: 	Q Alimentos e Nutrição Humana	
Registro original: 	Embrapa Agroenergia (CNPAE)	
Exemplares: 	CNPAE - (4313-1) - UPC - AP - DD -  -  -  - DIS