Data/hora: 04/06/2024 23:17:53

Biblioteca(s): | Embrapa Unidades Centrais.
Data corrente: | 07/10/2019
Data da última atualização: | 07/10/2019
Autoria: | OLIVEIRA JUNIOR, L. F. G. de; SANTOS, P. L. de S.; LIMA, R. S. N. de; SILVEIRA, M. P. C.; FAGUNDES, J. L.; GUTIERREZ CARNELOSSI, M. A.
Afiliação: | Luiz Fernando Ganassali de Oliveira Júnior, Universidade Federal de Sergipe - UFS; Patrícia Lima de Souza Santos, Universidade Federal de Sergipe - UFS; Roberta Samara Nunes de Lima, Universidade Federal de Sergipe - UFS; Maria Priscilla Celestino Silveira, Universidade Federal de Sergipe - UFS; Jailson Lara Fagundes, Universidade Federal de Sergipe - UFS; Marcelo Andrade Gutierrez Carnelossi, Universidade Estadual do Maranhão - UEMA.
Título: | Physiological parameters of cowpea treated with CaO-based particle film and subjected to water restriction.
Ano de publicação: | 2019
Fonte/Imprenta: | Pesquisa Agropecuária Brasileira, v. 54, e00033, 2019.
Idioma: | Inglês
Notas: | Título em português: Parâmetros fisiológicos de feijão-caupi tratado com filme de partícula de CaO e submetido à restrição hídrica.
Conteúdo: | The objective of this work was to evaluate the effects of CaO-based particle film on the physiological parameters of cowpea (Vigna unguiculata) subjected to water restriction. Plants were subjected to two levels of soil moisture and three concentrations of the film, as follows: control, without film + 100% crop evapotranspiration (ETc); without film + 50% ETc; 5% CaO + 50% ETc; 10% CaO + 50% ETc; 5% CaO + 100% ETc; and 10% CaO + 100% ETc. Plants treated with 50% ETc remained stable with the application of 10% CaO particle film and showed high photosynthetic assimilation of CO2 (32 &#956;mol m-2 s-1), moderate transpiration (5.6 mmol m-2 s-1), maintenance of chlorophyll content, and greater intrinsic water-use efficiency (IWUE, 226.65 &#956;mol mol-1) and instantaneous water-use efficiency (6.06 &#956;mol mmol&#8209;1) than plants of the other treatments. Control plants and plants at 5% CaO + 50% ETc showed, respectively, photosynthetic assimilation of CO2 at 15.34 and 15.94 &#956;mol m-2 s-1, transpiration at 3.51 and 3.45 mmol m-2 s-1, and IWUE at 177.7 and 198.9 &#956;mol mol-1. The CaO-based particle film is effective in protecting bean plants subjected to water restriction.
Palavras-Chave: | Troca gasosa; Water deficiency.
Thesagro: | Cálcio; Deficiência Hídrica; Vigna Unguiculata.
Thesaurus Nal: | Calcium; Gas exchange.
Categoria do assunto: | --
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/202609/1/Physiological-parameters-of-cowpea-treated.pdf
Registro original: | Embrapa Unidades Centrais (AI-SEDE)
Exemplares: | AI-SEDE - (64178-1) - UPE - AP - DD -  -  -  - DIS