Data/hora: 06/06/2024 03:47:59

Biblioteca(s): 	Embrapa Meio-Norte.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 2	
Data corrente: 	11/05/2022	
Data da última atualização: 	11/05/2022	
Autoria: 	REIS FILHO, R. J. C. dos; CARNEIRO, M. S. de S.; PEREIRA, E. S.; FURTADO, R. N.; MORAIS NETO, L. B. de; MAGALHAES, J. A.; ALVES, F. G. da S.; LOPES, M. N.	
Afiliação: 	RAIMUNDO JOSÉ COUTO DOS REIS FILHO, UFC, Fortaleza.; MARIA SOCORRO DE SOUZA CARNEIRO, UFC, Fortaleza.; ELZANIA SALES PEREIRA, UFC, Fortaleza.; RAFAEL NOGUEIRA FURTADO, IFPI, Paulistana, PI.; LUIZ BARRETO DE MORAIS NETO, Integral Agroindustrial Ltda, Fortaleza, CE.; JOAO AVELAR MAGALHAES, CPAMN; FRANCISCO GLEYSON DA SILVEIRA ALVES, UFC, Fortaleza.; MARCOS NEVES LOPES, IFPI, Valença do Piauí.	
Título: 	Biomass components and water use efficiency in cactus pear under different irrigation systems and harvest frequencies.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Revista Brasileira de Zootecnia, v. 51, e20210093, 2022.	
ISSN: 	1806-9290	
DOI: 	10.37496/rbz5120210093	
Idioma: 	Inglês	
Conteúdo: 	The objective was to evaluate the effect of different irrigation systems and harvest frequencies on the cultivation of cactus pear. The study was conducted in the semi-arid region, in the municipality of Russas, CE, Brazil. The experiment was a split plot randomized block design, with four replications. Plots were represented by irrigation systems (surface drip, microsprinkler, Micro Spray Jet, and conventional sprinkler) and subplots by harvest frequencies (6, 9, 12, and 18 months). Cactus pear biomass production characteristics were evaluated. Most of the productive characteristics evaluated were influenced by harvest frequency and irrigation system. The harvest frequency of 12 months combined with conventional sprinkler system resulted in a total dry biomass production of 16,400 kg ha&#8722;1. The conventional sprinkler system showed the highest number of second-order cladodes (4.9 cladodes plant&#8722;1). The conventional sprinkler and Micro Spray Jet systems showed the highest values for various structural characteristics. For water use efficiency (WUE), the highest value was found at the frequency of six months (8.46 kg ha&#8722;1 mm&#8722;1). Regarding the effects of irrigation system on WUE, the highest values were observed with the conventional sprinkler system (8.20 kg ha&#8722;1 mm&#8722;1). The harvest frequency of 12 months combined with the conventional sprinkler system presents better results in the evaluated productive characteristics, mainly the cactus pear production by area.	
Thesagro: 	Forragem; Irrigação; Manejo de Água.	
Thesaurus Nal: 	Cladodes; Forage production; Irrigation management; Opuntia stricta.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1142887/1/BiomassComponentsWaterEfficiencyCactusRBZ51.2022.pdf	
Registro original: 	Embrapa Meio-Norte (CPAMN)	
Exemplares: 	CPAMN - (33298-1) - UPC - AP - DD -  -  -  - DIS