Data/hora: 12/06/2024 16:23:58

Biblioteca(s): 	Embrapa Suínos e Aves.	
Data corrente: 	17/04/2015	
Data da última atualização: 	17/04/2015	
Autoria: 	SABINO, L. A.; ABREU, P. G. de; SOUSA JÚNIOR, V. R. de; ABREU, V. M. N.; COLDEBELLA, A.	
Afiliação: 	LUANA ARAÚJO SABINO, UNICAMP; PAULO GIOVANNI DE ABREU, CNPSA; VILMAR RODRIGUES DE SOUSA JÚNIOR, UNICAMP; VALÉRIA MARIA NASCIMENTO ABREU, CNPSA; ARLEI COLDEBELLA, CNPSA.	
Título: 	Interferência do material de construção na temperatura do ar no interior do escamoteador.	
Ano de publicação: 	2014	
Fonte/Imprenta: 	In: SEMINÁRIO INTERNACIONAL DE AVES E SUÍNOS, 15.; SEMINÁRIO TÉCNICO CIENTÍFICO DE AVES E SUÍNOS; FEIRA DA INDÚSTRIA LATINO-AMERICANA DE AVES E SUÍNOS, 2014, Florianópolis. Anais... Florianópolis: Gessulli, 2014. AVESUI 2014.	
Idioma: 	Português	
Conteúdo: 	O desenvolvimento dos leitões na maternidade constitui-se um fator determinante para o sucesso econômico na granja. Dessa forma, objetivou-se avaliar o conforto térmico de dois escamoteadores diferentes para leitões. Foi utilizada uma sala com quatro celas parideiras individual, sendo dois escamoteadores de madeira e dois de polietileno. No interior de cada escamoteador e no centro geométrico de cada sala foi instalado um datalogger de temperatura e umidade. Os dados foram coletados em quatro lotes durante três semanas a cada 30 minutos. Essas variáveis foram analisadas, por meio do modelo de medidas repetidas. O escamoteador de polietileno foi mais adequado com 27,36 % e 27,19 % dos dados dentro da faixa de conforto, enquanto o de madeira obteve 13,61% e 23,85% nas semanas 1 e 2 respectivamente. Somente na terceira semana o escamoteador de madeira obteve melhores resultados com 42,45% enquanto o de polietileno obteve 16,52% dos dados dentro da faixa de conforto. Ambos os escamoteadores obtiveram bons resultados quanto a umidade, obtendo média de dados dentro da faixa ideal de 58,30% o de polietileno e 69,85%, o de madeira. Piglet development in the farrowing house is a determining factor for the economic success the farm. The objective was to evaluate the thermal comfort of two different creeps for piglets. For this, it was used a farrowing house with four individual cells, twomade of wood, and two ofpolyethylene. Inside each creep and at the geometric center of each room , a datalogger was installed for recording the temperature and humidity. Data were collected in four batches every 30 minutes for three weeks. These variables were analyzed using a repeated measures model. The polyethylene creep was the most suitable with 27.36 % and 27.19% of the data within the comfort range, while the wooden creep achieved 13.61 % and 23.85% , in the weeks 1 and 2, respectively. Only on the third week the wood creep presented better results, with 42.45%, whereas that of polyethylene attained 16.52% of the data within the comfort rang. Both creeps achieved satisfactory results for the humidity, reaching mean values within the appropriate range, 58.30% and 69.85%, for polyethylene and wood creeps, respectively.	
Palavras-Chave: 	Arrowing; Edificação; Swines; Welfare.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/122465/1/final7656.pdf	
Registro original: 	Embrapa Suínos e Aves (CNPSA)	
Exemplares: 	CNPSA - (19952-1) - UPC - AA - DD -  -  -  - DIS