Data/hora: 25/05/2024 21:21:51

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	28/03/2005	
Data da última atualização: 	28/03/2005	
Autoria: 	MARTINS, M. A.; FERREIRA, F. C.; JOB, A.; MATTOSO, L. H. C.	
Título: 	Propriedades mecânicas e dinâmico-mecânicas de compósitos de borracha natural reforçados com fibra de sisal.	
Ano de publicação: 	2003	
Fonte/Imprenta: 	In: CONGRESSO BRASILEIRO DE POLÍMEROS. 7., nov. 2003., Belo Horizonte, MG. Anais... São Carlos: Associação Brasileira de Polímeros, 2003. p. 650-651.	
Idioma: 	Português	
Conteúdo: 	Short-fiber/elastomer composites are a growing class of materials. One important aspect for composite manufacture is to achieve satisfactory adhesion between the fibers and the matrix. In this work, the effect of chemical modification (mercerization and acetylation) and the addition of bonding agents resorcinol/ hexamethylenetetramine on the performance sisal fibers, Agave sisalana variety, in natural rubber (RRIM 600 clone) composites was evaluated. The composites were studied by mechanical and dynamic mechanical properties. Results of tensile properties show that the addition of fibers enhanced the modulus ca. 120%. Glass transition temperature of composites increases from 60 °C to - 50 °C	
Palavras-Chave: 	Polímero.	
Thesagro: 	Fibra Vegetal.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8759-1) - UPC - SP - -- - PROCI-03.00104 -  - 2003.00104 - DIS