Data/hora: 06/06/2024 13:58:42

Biblioteca(s): | Embrapa Meio Ambiente; Embrapa Recursos Genéticos e Biotecnologia.
Tipo da produção científica: | Artigo em Periódico Indexado
Circulação/Nível: | A - 1
Data corrente: | 08/09/2023
Data da última atualização: | 08/09/2023
Autoria: | SILVA, J. do N.; MASCARIN, G. M.; LOPES, R. B.; FREIRE, D. M. G.
Afiliação: | JAQUELINE DO NASCIMENTO SILVA, UNIVERSIDADE FEDERAL DO RIO DE JANEIRO; GABRIEL MOURA MASCARIN, CNPMA; ROGERIO BIAGGIONI LOPES, Cenargen; DENISE MARIA GUIMARÃES FREIRE, UNIVERSIDADE FEDERAL DO RIO DE JANEIRO.
Título: | Production of dried Beauveria bassiana conidia in packed-column bioreactor using agro-industrial palm oil residues.
Ano de publicação: | 2023
Fonte/Imprenta: | Biochemical Engineering Journal, v. 198, article 109022, 2023.
ISSN: | 1369-703X
DOI: | https://doi.org/10.1016/j.bej.2023.109022
Idioma: | Inglês
Conteúdo: | Abstract: Agro-industrial waste byproducts are commonly inexpensive organic nutritional sources for production of filamentous fungi, and selection of an optimal bioreactor is a key factor for attaining satisfactory biomass yield and quality. The insect-pathogenic fungus Beauveria bassiana (Hypocreales: Cordycipitaceae) has been extensively mass produced by solid-state fermentation using precooked cereal grains. Here, we propose low-cost palm oil residues as the main substrate using a cylindrical packed-column aerobic bioreactor prototype designed for conidial production of B. bassiana. Fermentation treatments using B. bassiana strain CG1229 assessed the impact of temperature, air flow, substrate moisture content, and ratio between palm fiber (PF) and palm kernel cake (PKC) on conidial yield and desiccation tolerance. Results showed significant enhanced productivity (2 ×1010 conidia g?1 dry matter) and reduced fermentation time (from 168 h to 120 h) by this method compared with the conventional tray bioreactor. Optimal substrate conditions were 60% initial moisture and 30% PF + 70% PKC content, fermentation at 26 °C with aeration rate ? 0.2 L min?1. Air drying conidia inside the column yielded > 95% germination. Maximum spore production was achieved in 120 h. Our findings demonstrate the feasibility of using a packed-column bioreactor for mass production of B. bassiana conidia using low-cost agricultural residues, which contributes to a sustainable production method of this biopesticide in Brazil.
Palavras-Chave: | Forced aeration; Waste valorization.
Thesagro: | Beauveria Bassiana; Elaeis Guineensis; Fermentação; Fungo Para Controle Biológico; Produção; Resíduo Orgânico.
Thesaurus Nal: | Biological control agents; biopesticides; Entomopathogenic fungi; Palm oils; Plant residues; Solid state fermentation.
Categoria do assunto: | H Saúde e Patologia
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1156508/1/Mascarin-Production-dried-2023.pdf
Registro original: | Embrapa Meio Ambiente (CNPMA)

Exemplares:

CNPMA - (17473-1) - UPC - AP - DD -  -  -  - DIS
CENARGEN - (39233-1) - UPC - AP - DD -  -  -  - DIS