Data/hora: 02/06/2024 14:25:25

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 23/01/2006
Data da última atualização: | 23/01/2006
Autoria: | MEDEIROS, E. S. de; BERNARDES FILHO, R.; MARTINEZ, R. A. de; GREGÓRIO FILHO, R.; MATTOSO, L. H. C.
Título: | Atomic force microscopy (AFM) of cured self assembled films.
Ano de publicação: | 2005
Fonte/Imprenta: | In: LATIN AMERICAN SYMPOSIUM ON SCANNING PROBE MICROSCOPY, 3., 2005, Ouro Preto. [Resumos...]. Ouro Preto: SBMN, 2005. 1 CD-ROM.
Idioma: | Inglês
Conteúdo: | Ultrathin films of conducting polumers are fundamental parts of many devices such as sensors due to many interesting properties which this class of materials exhibits (1-3). The sensoactive properties, i.e., the ability of a given conducting polymer in changing its transducing properties due to the presence of chemical species in the analyte are dependent , on the characteristics of film itself, such as porosity, roughness, thickness, etc.
Palavras-Chave: | AFM; Poly(o-ethoxyaniline); Sensors.
Thesaurus Nal: | polymers.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9225-1) - UPC - SP - -- - PROCI-05.00068 -  - 2005.00068 - DIS