Data/hora: 08/06/2024 20:21:08

Biblioteca(s): 	Embrapa Gado de Leite.	
Data corrente: 	03/05/2022	
Data da última atualização: 	03/05/2022	
Autoria: 	MENDONÇA, H. V. de; OTENIO, M. H.; LOMEU, A. A.; RITA, A. V. S.	
Afiliação: 	HENRIQUE VIEIRA DE MENDONÇA, Universidade Federal Rural do Rio de Janeiro; MARCELO HENRIQUE OTENIO, CNPGL; ALICE AZEVEDO LOMEU, Universidade Federal Rural do Rio de Janeiro; AMANDA VIEIRA SANTA RITA, Universidade Federal Rural do Rio de Janeiro.	
Título: 	Post-treatment of an aerated facultative pond with constructed wetland: first two years of operation in a dairy industry.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Ecological Engineering, v. 179, 106623, 2022.	
DOI: 	https://doi.org/10.1016/j.ecoleng.2022.106623	
Idioma: 	Inglês	
Conteúdo: 	In the present study, a horizontal subsurface flow constructed wetland (HSF-CW) with a surface area of 240 m2 and HRT of 2 days, was used in the post treatment of a facultative aerated pond. Application rates of 175 kg BOD5 ha? 1 day? 1 and 408 kg COD ha? 1 day? 1 can be considered admissible for HSF-CW operation following a facultative aerated pond. The system presented values for COD, BOD5 and TSS removal of 88%, 98.8% and 99.3%, respectively. The system supported operation at a solids application rate of 23.3 g TSS m? 2 day? 1 for two years without clogging. The species grown in the CW (Brachiaria ruziziensis) presented a biomass produtivity of between 1.86 and 2.55 kg m? 2 y? 1 , providing CO2 biofixation of between 3.10 and 3.98 kg m? 2 y? 1 . The present study, conducted over two years, indicates that the HSF-CW model employed, and the operational parameters proposed, can be used in post treatment for a pond system that is not operating satisfactorily.	
Thesagro: 	Capim Brachiaria; Impacto Ambiental; Indústria; Laticínio; Pântano.	
Categoria do assunto: 	L Ciência Animal e Produtos de Origem Animal	
Registro original: 	Embrapa Gado de Leite (CNPGL)	
Exemplares: 	CNPGL - (25627-1) - UPC - AP - DD -  -  -  - DIS