Data/hora: 06/06/2024 09:08:37

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 23/03/2006
Data da última atualização: | 31/07/2009
Autoria: | PEDROTTI, A.; CRESTANA, S.; CRUVINEL, P. E.; NAIME, J. M.; VAZ, C. M. P.
Título: | Calibration procedures of an X and gamma-rays tomography scanner for bulk density and moisture content studies of an albaqualf.
Ano de publicação: | 0
Fonte/Imprenta: | 4 f. Trabalho apresentado no 14 º Congresso Latinoamericano de la Ciencia del Suelo - CLACS-99, Temuco, Chile. Digitado.
Idioma: | Inglês
Conteúdo: | The X and gamma-rays tranmission computerized tomography (CT), process of obtaining the reconstructed image of an internal transverse section or slice of a body through a computer, using an external equipment. This technique allows to measure the bulk density and the water content of soil samples. The objective of this work is to describe calibration procedures of the CT scanner applied to bulk density and soil moisture studies in a Planossol (Albaqualf) from an experimental plot in Pelotas, Rio Grande do Sul State, southern Brazil.
Palavras-Chave: | Computerized Tomography; Planosol - Albaqualf; Soil Bulk density.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9642-1) - UPC - SP - -- - PROCI-99.00123 -  - 1999.00123 - DIS