Data/hora: 07/06/2024 09:44:23

Biblioteca(s): 	Embrapa Meio-Norte.	
Data corrente: 	05/09/2012	
Data da última atualização: 	18/12/2023	
Autoria: 	ANDRADE JUNIOR, A. S. de; BASTOS, E. A.; AGUIAR NETTO, A. O.; BRAGA, D. L.; SILVA, M. E.; NOLETO, D. H.	
Afiliação: 	ADERSON SOARES DE ANDRADE JUNIOR, CPAMN; EDSON ALVES BASTOS, CPAMN; ANTENOR O. AGUIAR NETTO, SERGIPE FEDERAL UNIVERSITY; DARLAN L. BRAGA, CEARA FEDERAL UNIVERSITY; MARIA E. SILVA, PIAUI FEDERAL UNIVERSITY; DONAVAN H. NOLETO, PIAUI FEDERAL UNIVERSITY.	
Título: 	Agricultural water footprint of ethanol and sugar from sugar cane under fertigation production system.	
Ano de publicação: 	2012	
Fonte/Imprenta: 	In: INTERNATIONAL CONFERENCE OF AGRICULTURAL ENGINEERING, 2012, Valencia. Agriculture & engineering for a healthier life: abstracts. Valencia: CIGR: EurAgEng, 2012.	
Idioma: 	Inglês	
Conteúdo: 	The study has objective to calculate the green, blue and grey agricultural water footprint (WF) of ethanol and sugar produced from sugar cane, under subsurface fertigation production system, in Piauí State, Brazil. Sugar and ethanol production data in response to different irrigation levels (288, 492 and 675 mm), nitrogen fertigation (90, 113 and 160 kg ha-1 N ) and potassium (60 and 133 kg ha-1 of K2O) plus a control treatment (2,080 mm of rainfall, 75 kg N ha-1 and 75 kg ha-1 of K2O) were obtained from a trial under subsurface drip irrigation system, RB 867515 sugar cane variety, 1st ratoon, conducted in COMVAP - Sugar and Alcohol Inc., União county, Piauí State, Brazil. Under subsurface drip fertigation, the agricultural WF for sugar production ranged from 1,493 L kg-1 (1,175 L kg-1 - green water, 163 L kg-1 - blue water and 155 L kg-1 - grey water) to 1,172 L kg-1 (823 L kg-1 - green water, 267 L kg-1 - blue water and 83 L kg-1 - gray water). For ethanol production, the agricultural WF ranged from 2,081 L L-1 (1,638 L L-1 - green water, 227 L L-1 - blue water and 216 L L-1 - grey water) to 1,483 L L-1 (1,040 L L-1 - green water, 338 L L-1 - blue water and 105 L L-1 - grey water). Under non-irrigated condition, the agricultural WF for sugar production was 1,915 L kg-1 (1,763 L kg-1 - green water and 152 L kg-1 - grey water) and 2,658 L L-1 (2,448 L L-1 - water green and 211 L L-1 - grey water) for ethanol production. The agricultural WF for the ethanol production was superior to sugar production. Agricultural water footprint under fertigation was lower than that obtained under non-irrigated condition, and should be a recommended practice for increasing water productivity to sugar and ethanol production from sugar cane crop in the region evaluated.	
Palavras-Chave: 	Demanda de água; Irrigação por gotejamento subterrâneo.	
Thesagro: 	Bioenergia.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/65606/1/Agricultural7390001.pdf	
Registro original: 	Embrapa Meio-Norte (CPAMN)	
Exemplares: 	CPAMN - (27456-1) - UPC - AA - PP - S 100/12 -  - 2012.00100 - DIS