Data/hora: 05/06/2024 08:11:50

Biblioteca(s): 	Embrapa Mandioca e Fruticultura.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 1	
Data corrente: 	10/02/2015	
Data da última atualização: 	09/03/2015	
Autoria: 	SILVA, A. J. P. da; COELHO, E. F.; COELHO FILHO, M. A.	
Afiliação: 	ALISSON JADAVI PEREIRA DA SILVA, IF Baiano; EUGENIO FERREIRA COELHO, CNPMF; MAURICIO ANTONIO COELHO FILHO, CNPMF.	
Título: 	Water extraction variability in the banana root zone affects the reliability of water.	
Ano de publicação: 	2015	
Fonte/Imprenta: 	Scientia Agricola, v.72, n.1, p.1-10, January/February 2015.	
ISSN: 	0103-9016	
Idioma: 	Inglês	
Conteúdo: 	Spatial and temporal variability of soil water extraction from the root zone affect soil water balance determination. The number of sensors installed in the root zone in studies addressing water balance is still set arbitrarily. This study provided an investigation of the water extraction process by banana (Musa spp.) roots by (i) determining the variability of water extraction from the banana tree root zone, (ii) detecting differences in the estimation of evapotranspiration (ET) by the soil water balance method when the number of soil profiles monitored in the roots zone varies, (iii) and; determining the minimum number of Time Domain Reflectometry (TDR) probes needed to obtain ET precision and accuracy similar to that determined by a drainage lysimeter. The field experiment was conducted in Cruz das Almas, in the state of Bahia, Brazil, where a drainage lysimeter was installed on a banana plantation. The water extraction in the banana root zone was quantified by the water content variations monitored in 72 points by TDRs, with measurements at 15-min intervals. The variability of water extraction in the banana root zone was medium to high. The range of variability affects the reliability of the crop evapotranspiration calculation by the soil water balance method. To prevent an overestimation of banana evapotranspiration, the water extraction in the soil profile must be monitored with at least 16 TDR probes installed at a minimum distance of 0.9 m and a minimum depth of 0.7 m. Keywords: soil moisture, soil water balance, water uptake	
Thesagro: 	Banana; Irrigação.	
Thesaurus Nal: 	Irrigation.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Mandioca e Fruticultura (CNPMF)	
Exemplares: 	CNPMF - (30454-1) - UPC - AP - PP -  -  -  - DIS