Data/hora: 07/06/2024 18:14:08

Biblioteca(s): 	Embrapa Instrumentação.	
Tipo da produção científica: 	Artigo em Periódico Indexado	
Circulação/Nível: 	A - 3	
Data corrente: 	18/04/2023	
Data da última atualização: 	12/01/2024	
Autoria: 	MALAFATTI, J. O. D.; TAVARES, F. A.; NEVES, T. R.; MASCARENHAS, B. C.; QUARANTA, S.; PARIS, E. C.	
Afiliação: 	ELAINE CRISTINA PARIS, CNPDIA.	
Título: 	Modified Silica Nanoparticles from Rice Husk Supported on Polylactic Acid as Adsorptive Membranes for Dye Removal.	
Ano de publicação: 	2023	
Fonte/Imprenta: 	Materials, v, 16, n. 6, 2429, 2023.	
Páginas: 	18 p.	
DOI: 	https://doi.org/10.3390/ma16062429	
Idioma: 	Inglês	
Conteúdo: 	Industrial effluents and wastewater treatment have been a mainstay of environmental preservation and remediation for the last decade. Silica nanoparticles (SiO2) obtained from rice husk (RH) are an alternative to producing low-cost adsorbent and agriculture waste recovery. One adsorption challenge is facilitating the adsorbate separation and reuse cycle from aqueous medium. Thus, the present work employs SiO2 supported on polylactic acid (PLA) nanofibers obtained by the electrospinning method for Rhodamine B (RhB) dye adsorption. The silica surface was modified with trimethylsilyl chloride (TMCS) to increase affinity towards organic compounds. As a result, the silanized surface of the silica from rice husk (RHSil) promoted an increase in dye adsorption attributed to the hydrophobic properties. The PLA fibers containing 40% SiO2 (w w&#8722;1 ) showed about 85?95% capacity adsorption. The pseudo-first-order kinetic model was demonstrated to be the best model for PLA:SiO2 RHSil nanocomposites, exhibiting a 1.2956 mg g&#8722;1 adsorption capacity and 0.01404 min&#8722;1 kinetic constant (k1 ) value. In the reuse assay, PLA:SiO2 membranes preserved their adsorption activity after three consecutive adsorption cycles, with a value superior to 60%. Therefore, PLA:SiO2 nanocomposites from agricultural waste are an alternative to ?low-cost/lowend? treatments and can be used in traditional treatment systems to improve dye removal from contaminated waters.	
Palavras-Chave: 	Electrospinning; PLA; Rice husk; Silica nanoparticles.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1153225/1/P-Modified-Silica-Nanoparticles-from-Rice-Husk-Supported-on.pdf	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (18217-1) - UPC - AP - DD - PROCI.23/32 -  - 2023/36 - DIS