Data/hora: 08/06/2024 14:13:19

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	30/03/2006	
Data da última atualização: 	24/08/2010	
Autoria: 	ASSIS, O. B. G.; VIEIRA, D. C.	
Título: 	Processing of open-pore glass membranes with defined pores form.	
Ano de publicação: 	2000	
Fonte/Imprenta: 	In: ANNUAL MEETING E EXPOSITION, 102., 2000, St. Louis. Annual meeting abstracts... Westerville: American Ceramic Society, 2000. p. 340.	
Idioma: 	Inglês	
Conteúdo: 	The development of open-pore glass membranes with defined pore geometry, suitable to enzyme immobilization, is processed following the efiller principleí. In this process an inorganic, non-sinterizable water-soluble phase, is admixed as pore-forming agents. After the heating cycle the salt is washed out forming a continuous porous structure.	
Palavras-Chave: 	AFM; Membranas; Open-pore; SEM.	
Thesagro: 	Enzima.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9701-1) - UPC - SP - -- - PROCI-00.00009 -  - 2000.00009 - DIS