Data/hora: 12/06/2024 01:59:37

Biblioteca(s): 	Embrapa Agroindústria de Alimentos.	
Data corrente: 	11/01/2022	
Data da última atualização: 	14/04/2022	
Autoria: 	CALIERO, C.; BIZZO, H. R.; RUBIOLO, P.; MARENGO, A.; GALLI, S.; ANDERSON, J. L.; SGORBINI, B.; BICCHI, C.	
Afiliação: 	CECILIA CAGLIERO, Università degli Studi di Torino; HUMBERTO RIBEIRO BIZZO, CTAA; PATRIZIA RUBIOLO, Università degli Studi di Torino; ARIANNA MARENGO; STEFANO GALLI, MEGA S. l. r.; JARED L. ANDERSON, Iowa State University; BARBARA SGORBINI, Università degli Studi di Torino; CARLO BICCHI, Università degli Studi di Torino.	
Título: 	Immobilization of phosphonium-based ionic liquid stationary phases extends their operative range to routine applications in the flavor, fragrance and natural product fields.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Journal of Chromatography A, v. 1664, n. 462796, 2022. 12 p. + 2 p. supl.	
DOI: 	https://doi.org/10.1016/j.chroma.2021.462796	
Idioma: 	Inglês	
Conteúdo: 	Phosphonium-based ionic liquids (ILs) have proven to be successful stationary phases (SPs) for gaschromatography (GC) in several fields of application because of their unique selectivity and good chromatographic properties. This study focuses on the use of two ILs as GC SPs that are based on the phosphonium derivatives trihexyl(tetradecyl)phosphonium chloride ([P66614+] [Cl−]), and tri-hexyl(tetradecyl)phosphonium bis[(trifluoromethyl)sulfonyl]imide ([P66614+][NTf2−]), which have previously been shown to be complementary in terms of chromatographic selectivity and retention. Their application in routine analysis has been limited by their lower maximum allowable operating temperatures (MAOT) (200 °C for the [P66614+][Cl−] IL and 180 °C for [P66614+][NTf2−]), which restricts their use to samples that consist of analytes with relatively high volatility. A previous study carried out in the Authors’ laboratory focused on extending the use of the [P66614+][Cl−] IL SP to the analysis of samples with analytes of medium-to-low volatility by optimizing column characteristics and operative conditions. This study addresses the immobilization of both the [P66614+][Cl−] and [P66614+][NTf2−] ILs to the inner wall of fused silica columns to increase their MAOT under soft and hard reaction conditions. The resulting MAOT depended on more or less drastic immobilization conditions, and reached 220 °C for soft immobilization (So-Im) and 240 °C for hard immobilization (Ha-Im) in the [P66614+][Cl−] IL columns, and 200 °C for So-Im and 220° for Ha-Im in columns coated with the [P66614+] [NTf2−] IL. The influence of immobilization on the separation power and performance of all the columns has been evaluated using i) the Grob test, ii) a model mixture of 41 compounds of different polarity, structure, and with different organic functional groups representative of the flavor and fragrance field, iii) a standard mixture of 37 fatty acid methyl esters, iv) the peppermint essential oil, v) two mixtures of sesquiterpenic alcohols (farnesols and santalols), and vi) a standard mixture of 16 pesticides. These test samples were also used to demonstrate the complementarity of the two phosphonium-based IL SPs in terms of selectivity and retention.	
Palavras-Chave: 	Column immobilization; Ionic liquid stationary phases; Operative conditions; Phosphonium-based ionic liquids.	
Thesaurus Nal: 	Gas chromatography.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Agroindústria de Alimentos (CTAA)	
Exemplares: 	CTAA - (15262-1) - UPC - AP - DD -  -  -  - DIS