Data/hora: 24/06/2024 21:59:56

Biblioteca(s): 	Embrapa Agroenergia.	
Data corrente: 	24/02/2014	
Data da última atualização: 	20/09/2017	
Autoria: 	ELKASABI, Y.; MULLEN, C. A.; PIGHINELLI, A. L. M. T.; BOATENG, A. A.	
Afiliação: 	Yaseen Elkasabi; Charles A. Mullen; ANNA LETICIA MONTENEGRO T PIGHINELL, CNPAE; Akwasi A. Boateng.	
Título: 	Hydrodeoxygenation of fast-pyrolysis bio-oils from various feedstocks using carbon-supported catalysts.	
Ano de publicação: 	2014	
Fonte/Imprenta: 	Fuel Processing Technology, v. 123, p. 11-18, 2014.	
DOI: 	doi.org/10.1016/j.fuproc.2014.01.039	
Idioma: 	Inglês	
Conteúdo: 	In this paper,we sought to elucidate the relationships between biomass feedstock type and the suitability of their fast-pyrolysis bio-oils for hydrodeoxygenation (HDO) upgrading. Switchgrass, Eucalyptus benthamii, and equine manure feedstocks were pyrolyzed into bio-oil using a continuous fast-pyrolysis system. We also synthesized variations of switchgrass bio-oil using catalytic pyrolysis methods (HZSM-5 catalyst or tail-gas recycle method). Bio-oil samples underwent batch HDO reactions at 320 °C under ~2100 psi H2 atmosphere for 4 h, using Pt, Ru, or Pd on carbon supports. Hydrogen consumption was measured and correlated with compositional trends. The resulting organic, aqueous, and gas phaseswere analyzed for their chemical compositions.Mass balances indicate little coke formation. Switchgrass bio-oil over Pt/C performed the best in terms of hydrogen consumption efficiency, deoxygenation efficiency, and types of upgraded bio-oil compounds. Eucalyptus feedstocks consistently consumed more than twice the normal amount of hydrogen gas per run, primarily due to the elevated syringol content. Catalytically pyrolyzed bio-oils deoxygenated poorly over Pt/C but hydrogenated more extensively than other oils. Although the relative deoxygenation (%DOrel) varied based on feedstock and catalyst, the absolute deoxygenation (%DOabs) depended only on the overall yield. The total extent of upgrading (hydrogenation+ deoxygenation) remained independent of feedstock and catalyst.	
Palavras-Chave: 	Bio-oil; Feedstock; Hydrotreating.	
Thesaurus Nal: 	biofuels; pyrolysis.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Agroenergia (CNPAE)	
Exemplares: 	CNPAE - (2410-1) - UPC - AP - DD -  -  -  - DIS