Data/hora: 06/06/2024 03:30:46

Biblioteca(s): 	Embrapa Clima Temperado; Embrapa Instrumentação.	
Data corrente: 	04/03/2024	
Data da última atualização: 	08/04/2024	
Autoria: 	AVILA, L. O. de; TORRES, D. P.; ORESTE, E. Q.; LISBOA, M. T.; SILVEIRA, C. A. P.; RIBEIRO, A. S.; NUNES, A. M.; MARTINAZZO, R.	
Afiliação: 	LIZIANE OLIVEIRA DE AVILA, UNIVERSIDADE FEDERAL DE PELOTAS; DAIANE PLACIDO TORRES, CNPDIA; ELIÉZER QUADRO ORESTE, UNIVERSIDADE FEDERAL DO RIO GRANDE; MEIBEL TEIXEIRA LISBOA, UNIVERSIDADE FEDERAL DE PELOTAS; CARLOS AUGUSTO POSSER SILVEIRA, CPACT; ANDERSON SCHWINGEL RIBEIRO, UNIVERSIDADE FEDERAL DE PELOTAS; ADRIANE MEDEIROS NUNES, UNIVERSIDADE FEDERAL DE PELOTAS; ROSANE MARTINAZZO, CPACT.	
Título: 	Speciation of Inorganic Arsenic in Retorted Oil Shale Slurry by Hydride Generation Atomic Absorption Spectrometry (HG AAS) after Ultrasound-Assisted Acid Extraction.	
Ano de publicação: 	2024	
Fonte/Imprenta: 	Analytical Letters, v. 57, n. 7, p. 1065-1077, 2024.	
DOI: 	https://doi.org/10.1080/00032719.2023.2240453	
Idioma: 	Inglês	
Conteúdo: 	An analytical method for determination of inorganic arsenic speciesin retorted oil shale slurry by atomic absorption spectrometrycoupled to hydride technique with ultrasound assisted acidic extrac-tion is reported. Trivalent arsenic measurement employed samplestabilization with a pH 4.5 prior to reaction with the reducing agentand analysis. In contrast, total inorganic As depended upon the pre-reduction of As(V) to As(III) with KI and ascorbic acid in 6.0 M HCland of As(V) was estimated by the difference of the total inorganicAs and As(III) concentrations. The limit of quantification was 3.7 mgkg1for As(III) and 1.3 mg kg1for itAs	
Thesagro: 	Arsênico; Espectrometria; Rocha; Xisto.	
Thesaurus Nal: 	Shale.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CPACT - (22798-1) - UPC - AP - DD -  -  -  - DIS
CNPDIA - (18404-1) - UPC - AP - DD - PROCI.24/23 -  - 2024/28 - DIS