Data/hora: 16/06/2024 06:15:26

Biblioteca(s): | Embrapa Solos.
Data corrente: | 06/01/2014
Data da última atualização: | 12/12/2016
Autoria: | SAMUEL-ROSA, A.; ANJOS, L. H. C. dos; VASQUES, G. de M.; ANTUNES, M. A. H.; DALMOLIN, R. S. D.
Afiliação: | Alessandro Samuel-Rosa, UFRRJ; Lúcia H. C. dos Anjos, UFRRJ; GUSTAVO DE MATTOS VASQUES, CNPS; Mauro A. H. Antunes, UFRRJ; Ricardo S. D. Dalmolin, UNIVERSIDADE FEDERAL DE SANTA MARIA.
Título: | Identifying and correcting oblique striping in the topodata digital elevation model.
Ano de publicação: | 2013
Fonte/Imprenta: | In: CONGRESSO BRASILEIRO DE CIÊNCIA DO SOLO, 34., 2013, Florianópolis. Anais... Florianópolis: Sociedade Brasileira de Ciência do Solo, 2013.
Idioma: | Inglês
Conteúdo: | The Topodata digital elevation model (DEM) is the best DEM available for digital soil mapping (DSM) in Brazil. However, it is not ready to use. We show that the kriging interpolator used to downscale the SRTM DEM from 3 arc-seconds to 1 arc-second spatial resolution increased the double oblique striping (15º and 60º) so common to SRTM DEMs. This is because kriging is quite sensitive to outliers. Besides, the Gaussian model of spatial covariance used in the downscaling enhanced the sensitivity of kriging to outliers, thus enhancing the striping. 2D Fast Fourier Transform can be used to identify whether a destriping procedure need to be employed. The bilinear or cubic resampling methods should be used to warp Topodata DEMs because they are insensitive to the double oblique striping.
Palavras-Chave: | 2D Fast Fourier Transform; DEM warping; SRTM downscaling.
Categoria do assunto: | P Recursos Naturais, Ciências Ambientais e da Terra
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/item/94694/1/identifying.pdf
Registro original: | Embrapa Solos (CNPS)
Exemplares: | CNPS - (17880-1) - UPC - AA - DD - 14.00008 -  - 14.00008 - DIS