Data/hora: 11/06/2024 18:21:58

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	13/09/2005	
Data da última atualização: 	13/09/2005	
Autoria: 	ASSIS, O. B. G.; FLORES, A. M.; BERNARDES-FILHO, R.; MASTELARO, V. R.	
Título: 	AFM surface characterization of Ce-oxide based porus glass for sensor applications.	
Ano de publicação: 	2001	
Fonte/Imprenta: 	Acta Microscopica, Maracaibo, v. 10, p. 87-90. abr 2001. Supplement 1. Proceedings of The First Latin American Symposium on Scanning Microscopy, São Pedro, SP, april, 2001.	
Idioma: 	Inglês	
Conteúdo: 	AFM was used to investigate pore formation in a Na-B-Nb-Ce glass by the leaching process. In the technique described, phase rich in B is formed within the matrix and removed by solubilization in boiling water. The resultant pores were measured using the statistical approach and presented medium size of aproximately 80 nm, irregularly distributed along the structure.	
Palavras-Chave: 	AFM; Microscopia de Força Atômica.	
Thesaurus Nal: 	biopolymers.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (8970-1) - UPC - SP - -- - PROCI-01.00065 -  - 2001.00065 - DIS