Data/hora: 15/06/2024 15:35:07

Biblioteca(s): | Embrapa Soja.
Data corrente: | 28/07/1993
Data da última atualização: | 13/10/2004
Autoria: | BOYD, A. H.
Título: | Drying soybeans for seed in the Southern United States.
Ano de publicação: | 1974
Fonte/Imprenta: | In: SOUTHEASTERN SOYBEAN PLANTING SEED SEMINAR, 1974, Mississippi. Proceedings. Mississippi State : Mississippi State University, 1974.
Páginas: | p.79-91.
Idioma: | Inglês
Conteúdo: | 1. High moisture soybeans can be harvested and dried and maintain adequate seed quality on an emergency basis, byt the quick drying required will place maximum pressure on the drying system and management and the margin for error is very low. 2. Pratically all grain drying systems can be used to dry soybean seed if precautions are taken to limit excessive drying and heat or mechanical damage. 3. An air flow of 9-12 cfm/bu is needed for sufficiently rapid drying at the top of the bins. 4. Temperature rise or heat applied should not result in a drying air RH less than 40%. 5. Too slow drying results in poor seed quality. 6. Too rapid or excessive drying results in poor seed quality. 7. No foolproof drying system exists. The operator must develop a working knowledge of the principles of drying and of his own drying systems.
Palavras-Chave: | Grain; Quality; Seed; Soybean.
Thesagro: | Dano Mecânico; Grão; Qualidade; Secagem; Semente; Soja.
Thesaurus Nal: | drying; mechanical damage.
Categoria do assunto: | --
Registro original: | Embrapa Soja (CNPSO)
Exemplares: | CNPSO - (7991-1) - ADD - PL - -- - 633.34 - S727p -  - DIS