Data/hora: 24/06/2024 20:08:34

Biblioteca(s): 	Embrapa Meio Ambiente.	
Data corrente: 	09/01/2024	
Data da última atualização: 	09/01/2024	
Autoria: 	BUENO, G.; BERNAL, F.; ROUBACH, R.; SKIPPER-HORTON, J. S.; SAMPAIO, F.; FIALHO, N.; BUREAU, D.	
Afiliação: 	GW BUENO, AQUACULTURE CENTER CAUNESP, SÃO PAULO STATE UNIVERSITY (UNESP), CAMPUS JABOTICABAL, 14884-900 JABOTICABAL, BRAZIL; FEM BERNAL, FACULTY OF AGRONOMY AND VETERINARY MEDICINE, UNIVERSITY OF BRASILIA (UNB), DARCY RIBEIRO CAMPUS - ICC SUL, ASA NORTE, 70910-900 BRASÍLIA, DF, BRAZIL; R ROUBACH, FISHERIES AND AQUACULTURE DEPARTMENT, FOOD AND AGRICULTURE ORGANIZATION OF THE UNITED NATIONS (FAO/UN), ROME 00153, ITALY; JO SKIPPER SKIPPER-HORTON, DEPARTMENT OF ANIMAL BIOSCIENCES, UNIVERSITY OF GUELPH, GUELPH, ON, N1G 2W1, CANADA; FG SAMPAIO, EMBRAPA ENVIRONMENT, BRAZILIAN AGRICULTURAL RESEARCH CORPORATION (EMBRAPA), ROD. SP 340, KM 127,5, CEP: 13.918-110, JAGUARIÚNA, SP, BRAZIL; NS FIALHO, AQUACULTURE CENTER CAUNESP, SÃO PAULO STATE UNIVERSITY (UNESP), CAMPUS JABOTICABAL, 14884-900 JABOTICABAL, BRAZIL; DP BUREAU, DEPARTMENT OF ANIMAL BIOSCIENCES, UNIVERSITY OF GUELPH, GUELPH, ON, N1G 2W1, CANADA.	
Título: 	Modeling of waste outputs in the aquatic environment from a commercial cage farm under neotropical climate conditions.	
Ano de publicação: 	2023	
Fonte/Imprenta: 	Aquaculture Environment Interactions, v. 15, p. 133-144, 2023.	
ISSN: 	1869-215X	
DOI: 	https://doi.org/10.3354/aei00457	
Idioma: 	Português	
Conteúdo: 	Abstract: The present study used a bioenergetics modeling approach to estimate the solid and dissolved waste outputs of a Nile tilapia <jats:italic>Oreochromis niloticus</jats:italic> net-cage farm. Historical production data for 30 cages were obtained from a commercial farm in the Chavantes Reservoir, São Paulo State, Brazil. In addition, an experiment was carried out in 4 net-cages at the farm to validate this dataset and collect fish samples. A total of 32400 tilapias with an initial weight averaging 35 ± 2.73 g were equally distributed in the experimental net cages. After 210 d, the fish showed a final individual weight of ~789 ± 5.12 g. Fish growth performance was monitored, and body composition was analyzed each month. Digestibility trials of commercial diets used for juvenile stages JVI and JVII and market weight were performed. Relationships of body weight with body content data of water, protein, fat, ash, gross energy, phosphorus, and nitrogen were evaluated by regression analysis. The total digestible energy requirement and estimated residues of the fish were assessed using the factorial bioenergetics model, adapted to the growing conditions of a neotropical reservoir. The model estimated ~320 kg of total solid waste released per tonne of tilapia, including ~10 kg of solid nitrogen and ~5 kg of solid phosphorus. Approximately 3 and 47 kg of dissolved phosphorus and nitrogen, respectively, were estimated per tonne of tilapia. The bioenergetics model is a valuable and equitable method for assessing and monitoring waste outputs. It can improve the nutritional and environmental efficiency of aquaculture activities, helping producers to reduce feed costs while strengthening the environmental sustainability of aquaculture.	
Palavras-Chave: 	Bioenergetics; Fish farm waste.	
Thesagro: 	Aquicultura; Dejeto; Resíduo Solido; Tilápia Nilótica.	
Thesaurus Nal: 	Aquaculture; carrying capacity; Tilapia (common name); Wastewater aquaculture.	
Categoria do assunto: 	L Ciência Animal e Produtos de Origem Animal	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1160595/1/Sampaio-modeling-waste-2023.pdf	
Registro original: 	Embrapa Meio Ambiente (CNPMA)	
Exemplares: 	CNPMA - (17561-1) - UPC - AP - DD -  -  -  - DIS