Data/hora: 22/09/2024 23:10:02

Biblioteca(s): 	Embrapa Agropecuária Oeste; Embrapa Cerrados; Embrapa Unidades Centrais.	
Data corrente: 	06/04/2006	
Data da última atualização: 	26/10/2009	
Autoria: 	MARTINS, E de S.; REATTO, A.; SILVA, A. V. da; FARIAS, M. F. R.; CARVALHO JÚNIOR, O. A. de; GUIMARÃES, R. F.	
Título: 	Geomorfologia da bacia hidrográfica do ribeirão Taguatinga, Distrito Federal, escala 1:25.000.	
Ano de publicação: 	2004	
Fonte/Imprenta: 	Planaltina, DF: Embrapa Cerrados, 2004.	
Páginas: 	38 p.	
Série: 	(Embrapa Cerrados. Boletim de Pesquisa e Desenvolvimento, 138).	
Idioma: 	Português	
Conteúdo: 	RESUMO A área selecionada para estudo foi a bacia hidrográfica do ribeirão Taguatinga (BHRT), Distrito Federal onde está localizada a Área de Relevante Interesse Ecológico Parque Juscelino Kubitschek (ARIE PARQUE JK), com área de 7.298,92 hectares, entre as coordenadas 15°30' e 15°40' S, e 47°50' e 48°12'W. Este estudo teve como finalidade caracterizar e mapear a geomorfologia da BHRT, em escala 1:25.000, para subsidiar o zoneamento ambiental e o plano de manejo d ARIE JK. Foram definidas unidades de mapeamento em três níveis hierárquicos, considerando as variáveis mais importantes para subsidiar estudos ambientais. No 1° nível, foram definidas as unidades: TOPOS DE CHAPADA (A), com 43,74% da área; RAMPAS (B), com 33,62% da área; ZONAS DE DISSECAÇÃO (C), com 22,64% da área. No 2° nível, foram definidasas unidades: Curso Superior (I), com 45,76% da área; Curso Médio (III), com 24,26% da área; Curso Inferior (III), com 29,98% da área. As unidades para o 3° nível são as seguintes: Topos Convexos (1), com 6,06% da área; Superfície Plano-Convexa das cabeceiras (2), com 21,07% da área; Superfície côncava-suave (3), com 5,73% da área; Superfície Plano-convexa do curso inferior (4), com 10,88% da área; Rampas suave-convexas e erosivas (5), com 30,45% da área. ABSTRACT The study was conducted at Taguatinga Stream - DF, located in the relevant ecological interest area Juscelino Kubitschek (ARIE - JK), and also in the Descoberto River, covering 7,298.92km2, located at 15°40'S and 47°50' and 48°12'W. The purpose was to characterise and map basin geomorphology, scale 1:25.000. Geomorphology units were defined in three hierarchical levels, considering the most important variables, to support environmental zoning and management planning. Three units were defined in the 2nd level: Superior Course (I), with 45.76%; Middle Course (II), with 24.26%; Inferior Course (III), with 29.98% of the area. The units for the 3rd level are: Convex tops (1), with 6.06%; Up stream flat-convex surface (2), with 21.07%; Soft concave surface (3), with 5.73%; Low Stream Flat-convex surface (4), with 10.88%; Soft Convex and Erosive Ramps (5), with 30.45%; Soft Concave and Colluvia Ramps (6), with 3.17%; Superior Dissected Zone (7), with 6.29%; Middle Dissected Zone (8), with 5.08%; Inferior Dissected Zone (9), with 5.37%; Alluvia Plain (10), with 1,50%; Colluvia-alluvia plain (11), with 0.16%; ribbed Depression (12), with 4.25%; Water Saturation Zones (13) superpose another units, with 14.40% of the area.	
Palavras-Chave: 	Classificação; Environmental zoning; Geormophology; Mapeamento; Relief; Zoneamento ambiental.	
Thesagro: 	Geomorfologia; Relevo; Solo.	
Thesaurus Nal: 	cartography; soil.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/CPAC-2009/26900/1/bolpd_138.pdf	
Registro original: 	Embrapa Cerrados (CPAC)	
Exemplares: 	AI-SEDE - (34877-1) - EMB - FL - -- - 08872 - CPAC - 08872a - DIS
AI-SEDE - (34877-2) - EMB - FL - -- - 08872 - CPAC - 08872 - DIS
CPAO - (27303-1) - EMB - FL - -- - FOL 14659 -  - FOL 14659 - DIS
CPAC - (26900-1) - UMT - FL - -- - FOL7615 -  - CRI6836 - DIS
CPAC - (26900-2) - UMT - FL - -- - FOL7615 -  - BPD138 - DIS
CPAC - (26900-3) - UMT - FL - -- - FOL7615 -  - FOL7615 - DIS