Data/hora: 24/06/2024 12:54:31

Biblioteca(s): | Embrapa Solos.
Data corrente: | 06/05/2024
Data da última atualização: | 06/05/2024
Autoria: | TAVARES, S. R. de L.; RODRIGUES, N. F.; CORRÊA, G. M.; HÜTHER, C. M.
Afiliação: | SILVIO ROBERTO DE LUCENA TAVARES, CNPS; NATÁLIA FERNANDES RODRIGUES, UNIVERSIDADE FEDERAL FLUMINENSE; GABRIELA MARTINS CORRÊA, UNIVERSIDADE FEDERAL FLUMINENSE; CRISTINA MOLL HÜTHER, UNIVERSIDADE FEDERAL FLUMINENSE.
Título: | Low-cost class a evapotranspiration pan for reference evapotranspiration estimation in protected and field environments: a practical approach.
Ano de publicação: | 2024
Fonte/Imprenta: | In: SILVA, L. F. da; GUEDES, D. M.; CRUSOÉ, J. M. S. F. (org.). Agricultural sciences unveiled: exploring the dynamics of farming and sustainability. Ponta Grossa: Atena, 2024. cap. 1, p. 1-9.
DOI: | https://doi.org/10.22533/at.ed.9662430041
Idioma: | Inglês
Conteúdo: | Currently, there are various methods for determining the Class A pan coefficient (Kp) in estimating reference evapotranspiration (ETo), which is of utmost importance for water management in agriculture. This study aimed to estimate ETo inside and outside agricultural greenhouses using a low-cost constructed Class A pan (TCA-c) method. To estimate ETo, it is necessary to establish the Kp, as ETo is the product of ECA multiplied by Kp. This study employed the calibration method, comparing ETo determined by Penman-Monteith (EToPM) with Class A pan evaporation (ECA) to determine Kp. EToPM served as the standard for correlations with reference evapotranspiration using the TCA-c method inside and outside an agricultural greenhouse, avoiding the installation of a "Class A" pan inside the greenhouse. The experiment was conducted at UFF's Gragoatá campus in Niterói - RJ. Four TCA-c pans were installed (three inside and one outside an agricultural greenhouse) and managed for one year. Principal Component Analyses (PCA) revealed significant differences in ETo throughout the seasons. Adjusted Kps were established for all pans. It was observed that ETo inside the greenhouse was lower than that estimated outside. It is recommended to install the TCA-c pan inside the greenhouse for ETo estimation, utilizing different Kps throughout the seasons.
Palavras-Chave: | Class A Pan; Pan coefficient.
Thesagro: | Evapotranspiração.
Thesaurus Nal: | Evapotranspiration.
Categoria do assunto: | P Recursos Naturais, Ciências Ambientais e da Terra
URL: | http://ainfo.cnptia.embrapa.br/digital/bitstream/doc/1164085/1/Low-cost-class-a-evapotranspiration-pan-2024.pdf
Registro original: | Embrapa Solos (CNPS)
Exemplares: | CNPS - (21461-1) - UPC - PL - DD -  -  -  - DIS