Data/hora: 19/06/2024 16:57:55

Biblioteca(s): 	Embrapa Pecuária Sudeste.	
Data corrente: 	04/10/2010	
Data da última atualização: 	30/06/2023	
Autoria: 	GROMBONI, C. F.; DONATI, G. L; MATOS, W. O.; NEVES, E. F. A.; NOGUEIRA, A. R. de A.; NOBREGA, J. A.	
Afiliação: 	CAIO F. GROMBONI, UFSCar/SÃO CARLOS, SP; GEORGE L. DONATI, UFSCar/SÃO CARLOS, SP; WLADIANA O. MATOS, UFSCar/SÃO CARLOS, SP; EDUARDO F. A. NEVES, UFSCar/SÃO CARLOS, SP; ANA RITA DE ARAUJO NOGUEIRA, CPPSE; JOAQUIM A. NÓBREGA, UFSCar, SÃO CARLOS, SP.	
Título: 	Evaluatin of metabisulfite and a commercial stee wool for removing chromium (VI) from wastewater.	
Ano de publicação: 	2010	
Fonte/Imprenta: 	Enviromental Chemistry Letter, v. 8, p.73-77, 2010.	
DOI: 	11110.1007/s0311-008-0194-6	
Idioma: 	Português	
Conteúdo: 	Efficiency of metabisulfite and a commercial steel wool as reducing agents in the removal of Cr(VI) from wastewaters was evaluated. Chromium( VI) was converted to Cr(III), precipitated with NaOH, and removed by filtration. A reduction of more than 1.0 x 10(5) and 4.0 x 10(5) fold in total Cr and the Cr(VI) concentrations, respectively, was observed by employing steel wool masses as low as 0.4420 g to 30-mL solutions of wastewater. Chromium(III) hydroxide obtained after the treatment was recycled and used as marker in cattle nutrition studies. The liquid residue obtained after the treatment was reused as precipitation agent replacing NaOH.	
Palavras-Chave: 	Metabisulfite; Steel wood.	
Thesaurus Nal: 	wastewater treatment.	
Categoria do assunto: 	W Química e Física	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/28784/1/ana2010.pdf	
Registro original: 	Embrapa Pecuária Sudeste (CPPSE)	
Exemplares: 	CPPSE - (19507-1) - UPC - AP - DD - PROCI-2010.00071 - GRO - 2010.00071 - DIS