Data/hora: 24/06/2024 20:39:06

Biblioteca(s): 	Embrapa Agroindústria de Alimentos.	
Data corrente: 	24/09/1998	
Data da última atualização: 	22/02/2011	
Autoria: 	ROSA, M. F.; ALBUQUERQUE, R. T.; FERNANDES, J. M. O.; LEITE, S. G. F.; MDRONHO, R. A.	
Título: 	Nitrification of saline effluents.	
Ano de publicação: 	1997	
Fonte/Imprenta: 	Brazilian Journal of Chemical Engineering, v.14, n.2, p.151-156, jun. 1997.	
Idioma: 	Inglês	
Conteúdo: 	An a crated submergel biological filter was used to promote biological nitrification of a synthetic saline waste water. Black PVC corrugated plates were used to make the structured packing of the 6 litter reactor. Nitrate, nitrite, and ammonia concentrations pH and do were periodically measured, according to APHA (1985).In spite of the deleterious effect of salinity.It was possible to obtain nitrogen removal efficiencies as high as 95% for a 25 g/L sal concentration after a three-day reaction in the batch reactor. Continuous operation using a NaCI concentration of 25 g/L was tested using three different hydraulic retention times: 7,15 and 25 hours. An increase in ammonia removal was observed when the retention time was increased from 7 to 15 hours. However, on further notable increase was obtained for a 25 hour retention time, showing that nitrogen removal tends towards a maximum limit of about 80%.	
Palavras-Chave: 	Nitrificacao: Saline wastewater; Residuos.	
Thesagro: 	Água Salgada.	
Thesaurus Nal: 	nitrification.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Agroindústria de Alimentos (CTAA)	
Exemplares: 	CTAA - (859-1) - UPC - AP - PP - CTAA-0088 -  - 1998.00038 - DIS