Data/hora: 06/06/2024 02:41:29

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	23/06/2021	
Data da última atualização: 	16/08/2022	
Autoria: 	LIMA, E. M. B.; MIDDEA, A.; MARCONCINI, J. M.; CORRÊA, A. C.; PEREIRA, J. F.; GUIMARÃES, A. V.; LIMA, J. F. de; ANJOS, M. R. dos; CASTRO, I. M. de; OLIVEIRA, R. N.; MOREIRA, C. R.; PAIVA, M. M. de; RANGEL, F. L. C.; NEUMANN, R.	
Afiliação: 	EDLA MARIA BEZERRA LIMA, CTAA; ANTONIETA MIDDEA, Centro de Tecnologia Mineral (CETEM); JOSE MANOEL MARCONCINI, CNPDIA; ANA CAROLINA CORRÊA, Universidade Federal de São Carlos (UFSCar); JÉSSICA FERNANDES PEREIRA; ALESSANDRA VIEIRA GUIMARÃES, UFRJ; JOSIMAR FIRMINO DE LIMA, Centro de Tecnologia Mineral (CETEM); MARIANNA RAMOS DOS ANJOS, CTAA; IZABELA MIRANDA DE CASTRO, CTAA; RENATA NUNES OLIVEIRA, Universidade Federal Rural do Rio de Janeiro (UFRRJ); CARLA RAMOS MOREIRA, Instituto Nacional de Tecnologia (INT); MAURÍCIO MAGALHÃES DE PAIVA, Instituto Nacional de Tecnologia (INT); FRANCISCO LUIZ CORREA RANGEL, Instituto Nacional de Tecnologia (INT); REINER NEUMANN, Centro de Tecnologia Mineral (CETEM).	
Título: 	Biodegradable PLA based nanocomposites for packaging aplications: The effects of organo-modified bentonite concentration.	
Ano de publicação: 	2021	
Fonte/Imprenta: 	Journal of Applied Polymer Science, v. 138, n. 36, 2021.	
Páginas: 	1-17	
DOI: 	https://doi.org/10.1002/app.50907	
Idioma: 	Inglês	
Conteúdo: 	The effects of concentration and surface modification of two Brazilian bentonite clays on nanocomposites' properties based on polylactic acid ? (PLA) were investigated. The samples were prepared by the extrusion/injection method to obtain biodegradable packaging plastics. The raw materials and their bionanocomposites were characterized by various techniques. Natural clay samples presented a size of around 2 ?m while the modified ones' size was 5?6 ?m, probably due to the presence of cetyltrimethylammonium bromide in the interlayer space. The particle size and the contact angle increased with the treatment and the clay's density decreased. The organoclays were homogeneously dispersed in PLA, which can be associated with the interactions between PLA chains' carbonyl groups and the organoclays. The bionanocomposites present modified clay particles axis aligned to the flow direction of the extruder/injector. Chocolate organoclay acts as a nucleating agent to PLA crystal growth, increasing the sample's crystallinity, while Bofe organoclay interferes with the amorphous chain's mobility and diminishes the sample's crystallization. The addition of both organoclays to PLA diminished the sample's elongation at break and strength, although the organoclays increased the sample's Young modulus, even though Bofe organoclay is more active in PLA amorphous phase and Chocolate organoclay on the crystalline one.	
Palavras-Chave: 	Biodegradable; Biomaterials.	
Thesagro: 	Tecnologia de Alimento.	
Thesaurus Nal: 	Biocompatibility; Biodegradable products; Food technology; Packaging.	
Categoria do assunto: 	X Pesquisa, Tecnologia e Engenharia	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (17801-1) - UPC - AP - DD - PROCI.21/57 -  - 2021/57 - DIS