Data/hora: 16/06/2024 19:05:52

Biblioteca(s): 	Embrapa Solos.	
Data corrente: 	01/06/2012	
Data da última atualização: 	03/11/2021	
Autoria: 	MELLIGAN, F.; DUSSAN, K.; AUCCAISE, R.; NOVOTNY, E. H.; LEAHY, E. H.; HAYES, M. H. B.; KWAPINSKI, W.	
Afiliação: 	University of Limerick, Ireland; University of Limerick, Ireland; ETELVINO HENRIQUE NOVOTNY, CNPS; University of Limerick, Ireland; University of Limerick, Ireland; University of Limerick, Ireland.	
Título: 	Characterisation of the products from pyrolysis of residues after acid hydrolysis of miscanthus.	
Ano de publicação: 	2012	
Fonte/Imprenta: 	Bioresource Technology, v. 108, p. 258-263, Mar. 2012.	
DOI: 	https://doi.org/10.1016/j.biortech.2011.12.110	
Idioma: 	Inglês	
Conteúdo: 	Platform chemicals such as furfural and hydroxymethylfurfural are major products formed during the acid hydrolysis of lignocellulosic biomass in second generation biorefining processes. Solid hydrolysis residues (HR) can amount to 50 wt.% of the starting biomass materials. Pyrolysis of the HRs gives rise to biochar, bio-liquids, and gases. Time and temperature were variables during the pyrolysis of HRs in a fixed bed tubular reactor, and both parameters have major influences on the amounts and properties of the products. Biochar, with potential for carbon sequestration and soil conditioning, composed about half of the HR pyrolysis product. The amounts (11-20 wt.%) and compositions (up to 77% of phenols in organic fraction) of the bio-liquids formed suggest that these have little value as fuels, but could be sources of phenols, and the gas can have application as a fuel.	
Palavras-Chave: 	Bio-liquid; Biorefinery.	
Thesaurus Nal: 	acid hydrolysis; biochar; pyrolysis.	
Categoria do assunto: 	P Recursos Naturais, Ciências Ambientais e da Terra	
Registro original: 	Embrapa Solos (CNPS)	
Exemplares: 	CNPS - (16529-1) - UPC - AP - DD -  -  - 2012.00166 - DIS