Data/hora: 11/06/2024 22:21:04

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 30/03/2006
Data da última atualização: | 30/03/2006
Autoria: | BASSOI, L. H.; VAZ, C. M.; HOPMANS, J. W.
Título: | Evaluation of field installation procedures of segmented TDR probes.
Ano de publicação: | 2000
Fonte/Imprenta: | In: AMERICAN SOCIETY OF AGRONOMY ANNUAL MEETING, 92., Minneapolis. Abstracts... Minneapolis: American Society of Agronomy, 2000. p. 209.
Idioma: | Inglês
Conteúdo: | Three procedures to install TDR probes were tested in the field: 1 - using a auger to make a hole, mixing the collected soil with water to make a mud and filling the hole before probe pushing to improve soil-probe contact. 2- using a rod, thinner rhan the probe, to make the hole and then probes were pushed into the soil. 3- using a rod with the same size as the TDR probes to make the hole, and probes were pushed into the soil.
Palavras-Chave: | Rod; TDR.
Thesaurus Nal: | soil.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (9705-1) - UPC - SP - -- - PROCI-00.00013 -  - 2000.00013 - DIS