Data/hora: 22/09/2024 16:45:48

Biblioteca(s): 	Embrapa Instrumentação.	
Data corrente: 	13/03/2006	
Data da última atualização: 	13/03/2006	
Autoria: 	INNOCENTINI, M. D. M.; SALVINI, V. R.; MACEDO, A.; PANDOLFELLI, V. C.	
Título: 	Prediction of ceramic foams permeability using Ergun's equation.	
Ano de publicação: 	1999	
Fonte/Imprenta: 	Materials Research=Revista Brasileira de Materiais, São Carlos, v.2, n.4, p.283-289, Oct. 1999.	
Idioma: 	Inglês	
Conteúdo: 	Sic-Al2O3 ceramic foams with 30 to 75 pores per linear inch (ppi) were used to access the application of pore size obtained by image analysis to estimate the cellular materials permeability through Ergun's equation. Samples were sliced and the pore size distribution, cross-sectional porosity and pore density were evaluated as a function of the slice thickness based on optical and X-ray computerized tomography acquired images.	
Palavras-Chave: 	Ceramic foams; Ergun's equation.	
Thesaurus Nal: 	image analysis; permeability.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Instrumentação (CNPDIA)	
Exemplares: 	CNPDIA - (9569-1) - UPC - SP - -- - PROCI-99.00073 -  - 1999.00073 - DIS