Data/hora: 24/06/2024 21:44:29

Biblioteca(s): 	Embrapa Agropecuária Oeste.	
Data corrente: 	13/02/2023	
Data da última atualização: 	13/02/2023	
Autoria: 	LEITE, B. K. V.; ORRICO, A. C. A.; ORRICO JUNIOR, M. A. P.; ASPILCUETA BORQUIS, R. R.; TOMAZI, M.; OLIVEIRA, J. D. de; VILELA, R. N. da S.; SCHWINGEL, A. W.	
Afiliação: 	BRENDA KELLY VIANA LEITE, UNIVERSIDADE FEDERAL DA GRANDE DOURADOS; ANA CAROLINA AMORIM ORRICO; MARCO ANTONIO PREVIDELLI ORRICO JUNIOR, UNIVERSIDADE FEDERAL DA GRANDE DOURADOS; RUSBEL RAUL ASPILCUETA BORQUIS, UNIVERSIDADE TECNOLOGICA DO PARANÁ; MICHELY TOMAZI, CPAO; JULIANA DIAS DE OLIVEIRA, UNIVERSIDADE FEDERAL DA GRANDE DOURADOS; RANIELLE NOGUEIRA DA SILVA VILELA, UNIVERSIDADE FEDERAL DA GRANDE DOURADOS; ALICE WATTE SCHWINGEL, UNIVERSIDADE FEDERAL DA GRANDE DOURADOS.	
Título: 	Use of biochar and crude glycerin as additives in the composting of slaughterhouse waste in static piles.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Renewable Agriculture and Food Systems, v. 37, n. 3, p. 268 - 277, 2022.	
DOI: 	10.1017/S174217052100055710.1017/S1742170521000557	
Idioma: 	Inglês	
Conteúdo: 	This study is aimed to evaluate the efficiency of biochar and crude glycerin as additives in N retention throughout the composting of cattle slaughterhouse waste in static piles receiving forced aeration. There were five treatments (control, biochar accounting for 5 and 10%, and glycerin accounting for 5 and 10%, both at total solids) and four times (20, 50, 70 and 90 days of composting). The slaughterhouse waste was composted with a bulking agent at a ratio of 3:1, and the mixtures of waste and the tested additives were placed in nylon bags. The piles reached thermophilic temperatures soon after the process started and following turnings. The reductions of volatile solids, carbon, hemicellulose, cellulose and lignin were not influenced by the additives, resulting in averages of 69.1, 67.1, 62.1, 51.6 and 35.3%, respectively. The control showed greater N losses (58.38%), compared to the treatments with additives. The inclusions of biochar yielded an average loss of 48.47% N, while 10% of glycerin resulted in the lowest N losses (44.83%). The use of biochar and glycerin as additives in the composting of slaughterhouse waste is recommended in order to decrease N losses and improve the concentration of nutrients, without compromising the biodegradation of organic components.	
Thesagro: 	Aeração do Solo.	
Categoria do assunto: 	A Sistemas de Cultivo	
Registro original: 	Embrapa Agropecuária Oeste (CPAO)	
Exemplares: 	CPAO - (37344-1) - UPC - AP - DD -  -  -  - DIS