Data/hora: 22/09/2024 07:39:41

Biblioteca(s): 	Embrapa Clima Temperado.	
Data corrente: 	09/03/2022	
Data da última atualização: 	10/08/2022	
Autoria: 	RIBEIRO, P. L.; BAMBERG, A. L.; PEREIRA, I. dos S.; MONTEIRO, A. B.; POTES, M. da L.; LIMA, C. L. R. de.	
Afiliação: 	PABLO LACERDA RIBEIRO; ADILSON LUIS BAMBERG, CPACT; IVAN DOS SANTOS PEREIRA; ALEX BECKER MONTEIRO; MARIANA DA LUZ POTES; CLÁUDIA LIANE RODRIGUES DE LIMA.	
Título: 	Liming and co-application of water treatment residuals with biosolids for conditioning sandy soils.	
Ano de publicação: 	2022	
Fonte/Imprenta: 	Land Degradation and Development, v. 33, n. 7, p. 989-1001, 2022.	
DOI: 	10.1002/ldr.4202	
Idioma: 	Inglês	
Notas: 	First published: 17 January 2022.	
Conteúdo: 	Application of water treatment residuals (WTR) and biosolids (BS) might ameliorate fragile soils. However, studies integrating impacts of waste preparation methods such as liming and grinding associated with co-application approaches for soil conditioning are lacking. The present study aimed to evaluate the feasibility of agricultural use of WTR as well as their co-application with BS to ameliorate a sandy soil through assessing impacts on selected soil quality indicators and on nutrient and potentially toxic element concentration in plant tissue in addition to the biomass yield of annual crops. The following treatments were evaluated: non-amended soil (control); drying plus grinding and liming WTR; WTR co-application with BS at 3:1 ratio; and a soil amendment commercially available in Brazil. All treatments were soil incorporated in the 0.0?0.2 m layer at 30 Mg ha1 dose (dry mass). Selected soil physical, hydraulic, and chemical parameters were determined. Furthermore, nutrients and potentially toxic elements concentration in plant tissue as well as the agronomic performance of maize and ryegrass were measured. The co-application of WTR and BS increased the soil content of P, Zn, and Cu in the 0.0?0.1 m layer. The concentration of these nutrients also was greater in ryegrass tissue and promoted the biomass yield in 51%. WTR did not increase contaminants and did not decrease the P content in soil and in plant tissue, independently of drying plus grinding and liming. Considering the conditions investigated in our study, WTR/BS co-application was environmentally safe and effective in ameliorating soil quality.	
Thesagro: 	Água; Solo Arenoso; Tratamento da Água.	
Categoria do assunto: 	--	
URL: 	http://ainfo.cnptia.embrapa.br/digital/bitstream/item/232279/1/Artigo-Liming-and-co8208application-of-water-treatment-residuals-with-biosolids-for-conditioning.pdf	
Registro original: 	Embrapa Clima Temperado (CPACT)	
Exemplares: 	CPACT - (22190-1) - UPC - AP - DD -  -  -  - DIS