Data/hora: 25/06/2024 01:31:13

Biblioteca(s): 	Embrapa Mandioca e Fruticultura.	
Data corrente: 	02/12/1993	
Data da última atualização: 	04/04/2001	
Autoria: 	TESIC, M.; KISGECI, J.; MULLER, J.	
Afiliação: 	Institute for Agricultural Engineering.	
Título: 	Drying of medicinal plants in a greenhouse type solar dryer in yugoslavia	
Ano de publicação: 	0	
Fonte/Imprenta: 	Garbentrasse: s.d., 1p.	
Idioma: 	Inglês	
Conteúdo: 	A solar dryer for medicinal plants was developed on the basis of a plastic foil covered greenhouse. This dryer was tested in  Yusgoslavia in an area where medicinal plants are produce in large scale. To decrease the investment costs of the drying unit the solar air heater is incorporated into the roof of a greenhouse construction. The solar air heater consists of a transparent plastic cover foil, a black textile fabric and an air-bubble foil, which avoids heat losses on the back. The foils as well as the textile fabric are connected onto the construction by a special weather strip fixing system. To enlarge the area of the solar air heater, the roof is extended on the southern side almost to the ground. 	
Thesagro: 	Temperatura.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Mandioca e Fruticultura (CNPMF)	
Exemplares: 	CNPMF - (15411-1) - ADC - SP - -- - S905 -  - S905 - DIS
CNPMF - (18996-1) - ADC - SP - -- - S1905 -  - S1905 - DIS