Data/hora: 16/06/2024 09:56:07

Biblioteca(s): | Embrapa Instrumentação.
Data corrente: | 25/04/2003
Data da última atualização: | 25/04/2003
Autoria: | ALBUQUERQUE, J. E. de; MELO, W. L. B.; FARIA, R. M.
Afiliação: | Universidade Federal de Viçosa, Departamento de Física, Viçosa, MG; Embrapa Instrumentação Agropecuária, São Carlos, SP; USP-Instituto de Física de São Carlos, SP.
Título: | Determination of physical parameters of conducting polymrs by photothermal spectroscopies.
Ano de publicação: | 2003
Fonte/Imprenta: | Review of Scientific Instruments, Rochester, v. 74, n. 1, p. 306-308, Jan. 2003.
Idioma: | Inglês
Conteúdo: | Photothermal spectroscopies, photopyroelectric and photoacoustic, were used to obtain physical parameters of polyaniline-emeraldine base (PANI-EB) and poly(0-methoxyaniline)-emeraldine base (POMA-EB), such as thermic parameters like thermal diffusivity, thermal conductivity, and specific heat. These studies were done for PANI-EB and POMA-EB films in the 400<delta<900nm wavelength range. The photopyroelectric intensity Vn(f) and the phase Fn(f) (f being the chopping frequency) for a given delta of the saturation part of the PPES spectrum signal were independently measured, as well as the intensity Vn(delta) and its phase Fn(delta). Equations of both the intensity and the phase of the PES signal, taking into account the thermal and the optical characteristics of the PANI and POMA films and the pyroelectric detector, were used to fit the experimental results. It was observed that, in contrast with the strong doping dependence of the electrical conductivity, the thermal parameters of PANI films remained practically unchanged under doping. This apparent discrepancy is explained by the granular metal model of doped PANI.
Palavras-Chave: | Photoacoustic; Photopyroelectric; Photothermal spectroscopies; Polyaniline; Solid-state material.
Thesaurus Nal: | polymers.
Categoria do assunto: | --
Registro original: | Embrapa Instrumentação (CNPDIA)
Exemplares: | CNPDIA - (7443-1) - UPC - SP - -- - PROCI-03.00003 -  - 2003.00003 - DIS