Data/hora: 25/06/2024 06:15:29

Biblioteca(s): 	Embrapa Meio Norte / UEP-Parnaíba.	
Data corrente: 	06/05/1996	
Data da última atualização: 	06/05/1996	
Autoria: 	MANNERING, J. V.; MEYER, L. D.	
Título: 	The effect of various rates on surface mulch on infiltration and erosion.	
Ano de publicação: 	1970	
Fonte/Imprenta: 	Soil Science Society of America, v.27, p.84-86. 1970.	
Idioma: 	Inglês	
Conteúdo: 	The effects of six rates of applied wheat straw mulch on infiltration and erosion were studied on a highly permeable wea silt loam with 5% slope. Series of simulated rain storms totaling   6,25 inches at an intensity of 2.5 inches per hour were used to evaluate the treatments. Mulch  applications of 1,2 and 4 tons per acre maintained very high infiltration rates resulting in essentially no erosion. The 1/4 and 1/2 ton mulch application lost 3 tons and 1 ton of siol per acre, respectively, whereas the check (no mulch) treatment lost 12 tons per acre. Benefits which were indicated from the mulching were: 1) reduced soil surface sealing as evidenced by higher infiltration rates, and 2) decreased rainfall and runoff energy for particle detachment and transport asevidenced by reduced soil content in the runoff.	
Palavras-Chave: 	Erosion; Infiltration.	
Thesagro: 	Erosão; Infiltração; Solo.	
Thesaurus Nal: 	soil.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Meio Norte / UEP-Parnaíba (CPAMN-UEPP)	
Exemplares: 	CPAMN-UEPP - (5951-1) - ADP - SP - -- -  -  - 1988.00100 - DIS