Data/hora: 19/09/2024 23:06:30

Biblioteca(s): 	Embrapa Mandioca e Fruticultura.	
Data corrente: 	29/09/2000	
Data da última atualização: 	29/09/2000	
Autoria: 	MUHLBAUER, W.; MAIER, G.; BERGGOTZ, T.; ESPER, A.; QUICK, G. R.; MAZAREDO, T.	
Afiliação: 	Institue for Agric. Eng. in the Tropics and Subtropics Hohenheim University Stuttgart, Germany; International Rice Research Institute Los Banos, Philippines.	
Título: 	Low-temperature dryinf of paddy under humid tropical conditions.	
Ano de publicação: 	1992	
Fonte/Imprenta: 	Agricultural Mechanization in Asia, Africa and Latin America, v.23, n.4, p.33-41, 1992.	
Idioma: 	Inglês	
Conteúdo: 	A low-temperature dryng system for paddy consisting of a rectangular bin, an air sweep floor for air distribuition and unloading, an eletric heater and a centrifugal fan was tested dur ing the raing season in the Philippines during 1989 and 1990. The investigations showed that even during humid tropical weather conditions a layer of paddy up to 2 m thick can be dried from an initial moisture content as high as 27.5% w.b. in one step to a safe storange level. The bin, which is 1.8 m wide, 2.5 m long has a maximum capacity of tons at a bulk depth of 2.0 m,allows the yield of 1 ha to dried within 6 days. Low air flow and the use of a high efficient fan for forcing the air through the bulk yield the extremely low power requirement of 40 Watt per m3 of grain.                                                                                               	
Palavras-Chave: 	Aspecto socio-economico; Cultivares; Pos colheita; Regiao Tropical humido.	
Thesagro: 	Clima; Fungo.	
Categoria do assunto: 	--	
Registro original: 	Embrapa Mandioca e Fruticultura (CNPMF)	
Exemplares: 	CNPMF - (15362-1) - ADC - SP - -- - S1503 -  - S1503 - DIS