Data/hora: 19/06/2024 10:57:24

Biblioteca(s): | Embrapa Mandioca e Fruticultura.
Data corrente: | 28/09/2000
Data da última atualização: | 28/09/2000
Autoria: | KIM, K. S.; SHIN, M. G.; KIM, B. C.; RHIM, J. H.; CHEIGH, H. S.; MUHLBAUER, W.; KWON, T. W.
Afiliação: | Korea Advanced Institute for Scienced and Technology (KAIST) P.O.Box 131, Cheongyang Seoul, Korea; Pusan National Univ. 30 Jang Jang-Dong, Dong Lae-Ku. Pusan, Korea.
Título: | An ambient-air in-storange paddy drying system for Korean farms.
Ano de publicação: | 1989
Fonte/Imprenta: | Mechanization in Asia Africa and Latin America, v.20, n.2, p.23-29, 1989.
Idioma: | Inglês
Conteúdo: | An ambient-air in-storange paddy drying system for small scale Korean farms was developed and teste. Tris dryer consists of a rectangular container, an air distribuition system and a centrifugal fan. The system can be incorporated into either new or existing structures. When drying is finished the container can be used for storange purposes or as a machine shed. Depending on the dimensions of the container and the depth of the bulk, the loading capacity ranges from 3 to 5 t, which allowes application to fam sizes of 0.5 to 1.0 ha. Tje dryer can constructed by the famers themselves or craftsmen using locally available materials. Tests carried out in 1981 to 1985 showed that under Korean weather conditions, a layer of paddy 0.9 to 1.2 m thick can be dried with in 7 to 15 days from an initial moisture content of uo to 25% to safe storange conditions by continuous ventilation with ambient air.
Palavras-Chave: | Armazenagem; Aspecto economico.
Thesagro: | Agricultura; Clima; Energia.
Categoria do assunto: | --
Registro original: | Embrapa Mandioca e Fruticultura (CNPMF)
Exemplares: | CNPMF - (15363-1) - ADC - SP - -- - S1501 -  - S1501 - DIS