Data/hora: 29/05/2024 09:20:22

Biblioteca(s): 	Embrapa Agroindústria Tropical; Embrapa Alimentos e Territórios.	
Data corrente: 	30/04/2024	
Data da última atualização: 	30/04/2024	
Autoria: 	PAIVA, E. M. DE; MATTOS, A. L. A.; SILVA, G. S. DA; CANUTO, K. M.; LEITAO, R. C.; ALVES, J. L. F.; BRITO, E. S. de.	
Afiliação: 	EVANICE MEDEIROS DE PAIVA, FEDERAL UNIVERSITY OF CEARÁ; ADRIANO LINCOLN ALBUQUERQUE MATTOS, CNPAT; GISELE SILVESTRE DA SILVA; KIRLEY MARQUES CANUTO, CNPAT; RENATO CARRHA LEITAO, CNPAT; JOSE LUIZ FRANCISCO ALVES, FEDERAL UNIVERSITY OF PARAÍBA; EDY SOUSA DE BRITO, CNAT.	
Título: 	Valorizing cashew nutshell residue for sustainable lignocellulosic panels using a bio-based phenolic resin as a circular economy solution.	
Ano de publicação: 	2024	
Fonte/Imprenta: 	Industrial Crops and Products, 212, 118379, 2024.	
Idioma: 	Inglês
Português	
Conteúdo: 	he motivation for this study stems from the significant annual amount of cashew nutshells produced worldwide, which has raised growing concerns about proper environmental disposal. One alternative is to utilize the nutshells to produce particleboards and eco-friendly resin, thereby contributing to the circular economy. The present study proposes an innovation by providing the first insights into particleboard production, utilizing pressed cashew nutshell and a phenolic resin derived from the reaction of cashew nutshell liquid (CNSL) with formaldehyde. The mass proportions of CNSL to formaldehyde were varied at 1:0.25, 1:0.5, and 1:0.75 (w/w) without the necessity for isolating chemical compounds at 105 °C. The resin was characterized using rheology, DSC, FTIR, HPLC, and NMR techniques. The mechanical properties of the particleboard were evaluated through density, tensile, flexural, water absorption, and thickness swelling tests. The formaldehyde emission and biodegradability content of the particleboards were also evaluated. Eco-friendly phenol-formaldehyde resin promoted the modulus of elasticity (MOE) from 707 to 1866 MPa and the modulus of rupture (MOR) from 6.4 to 14.3 MPa. In addition, using adhesive with CNSL to formaldehyde mass ratios of 1:0.25 and 1:0.50 resulted in particleboards of class E1 in terms of formaldehyde emissions. The biodegradability of panels PB25, PB50 and PB75 was 30%, 21% and 20%, respectively, in 30 days. These findings demonstrate the potential of cashew nutshell biomass and eco-friendly resin as an adhesive in the particleboard industry.	
Palavras-Chave: 	Adesivo ecológico; Biodegradabilidade; CNSL; Eco-friendly adhesive; Emissão de formaldeído; Formaldehyde emission; LNC; Propriedades mecânicas.	
Thesagro: 	Desperdício.	
Thesaurus Nal: 	Biodegradability; Mechanical properties; Wastes.	
Categoria do assunto: 	--
W Química e Física	
Registro original: 	Embrapa Agroindústria Tropical (CNPAT)	
Exemplares: 	CNPAT - (17254-1) - UPC - AP - DD -  -  -  - DIS
CNAT - (127-1) - UPC - AP - DD -  - PAI -  - DIS